

Installation of **Bottom Rail** for Hi-Point 995 9mm w/ATI stock.

Always, always, always…read the instruction in full BEFORE starting the installation so as to be sure that you have a good understanding of the installation process.

OUR PICATINNY BOTTOM RAIL MOUNTS DIRECTLY TO THE RAISED BOSS AREA ON THE BOTTOM SECTION OF THE PLASTIC FORE-END AND INSTALLS USING THE SUPPLIED 3 SCREWS.

TO INSTALL:

1. ALWAYS BEGIN ANY INSTALLATION WITH THE GUN COMPLETELY UNLOADED.
2. ON THE BOTTOM MOUNT AREA OF THE PLASTIC STOCK FORE-END OF THE GUN, YOU ARE GOING TO POSITION THE NEW RAIL ONTO THE ANGLED LOWER FRONT SECTION OF THE ATI STOCK. NOTE: IF NO RAISED MOUNTING BOSS EXISTS ON YOUR PARTICULAR STOCK, YOU MAY HAVE TO USE TAPE TO TEMPORARILY SECURE THE RAIL INTO YOUR DESIRED POSITION UNTIL THE MOUNTING HOLES HAVE BEEN DRILLED OUT)
3. FIRMLY PUSH THE RAIL INTO PLACE ONTO THE RAISED PLASTIC BOSS (IF YOUR STOCK HAS THIS FEATURE)
4. USING THE NEW RAIL AS A GUIDE, CAREFULLY DRILL OUT THE 3 MOUNTING HOLES USING A 1/8” DRILL BIT.
5. INSTALL3 MOUNTING SCREWS AND TIGHTEN. TAKE CARE NOT TO OVERTIGHTEN.
6. MAKE SURE THAT RAIL IS FULLY SEATED ONTO THE STOCK.
7. THAT’S IT, YOU’RE DONE.
8. Got questions or are uncertain of the installation process, please call us at 973-786-4004 and we can guide you over the phone.

**www.LongShotMfg.com**