

Installation of **Black DELRIN Fore End Grip / Stock**

for **Chiappa LITTLE BADGER**

Always, always, always…read the instruction in full BEFORE starting the installation so as to be sure that you have a good understanding of the assembly process.

**Hardware Included:** 3mm x 5mm screws ( x3 ), 5/64 Hex Key

NOTE: Although it is not necessary, it is easier to ID certain parts during the installation if you have the Original Owners Manual open to the pages showing the gun assembly diagrams.

TO INSTALL:

1. **ALWAYS** CHECK THE CHAMBER AND BEGIN ANY INSTALLATION WITH THE GUN COMPLETELY UNLOADED!
2. USING THE SUPPLIED HEX KEY OR OTHER HEX / SPLINED BIT, UNSCREW THE 3 SCREWS THAT SECURE THE TOP AND SIDE PLASTIC RAILS TO THE GUN AND REMOVE THESE 3 RAILS.
3. POSITION NEW DELRIN FORE END GRIP SO THAT THE THREE BOTTOM SCREW HOLES LINE UP PROPERLY, INSERT THE 3 SUPPLIED SCREWS LOOSELY AND MAKE SURE THAT ALL SCREWS ARE THREADED INTO ALL HOLES BEFORE TIGHTENING, AND THEN **GENTLY** TIGHTEN EACH TO SECURE. **NOTE:** DO NOT OVERTIGHTEN OR DAMAGE TO THE FORE END GRIP COULD OCCUR. SCREWS SHOULD ONLY BE SNUG!
4. THAT’S IT, YOU’RE DONE. WE SUGGEST THAT YOU SAVE ALL REMOVED PARTS IN CASE YOU WISH TO RETURN GUN TO ORIGINAL FACTORY SET UP.

Got questions?.. or are uncertain of the installation process, please call us at 973-786-4004 and we can guide you over the phone.