

**Installation of INTEGRATED SHROUD / RAIL for Hi-Point 4595TS, 4095TS and 995TS.**

.

OUR PICATINNY INTEGRATED SHROUD - RAIL MOUNTS DIRECTLY TO BARREL AN SELF ALIGNS BY INSERTING ITS KEYED END INTO THE SQUARE OPENING OF THE PLASTIC STOCK FORE-END JUST BENEATH THE BARREL. THE SHROUD INSTALLS USING THE PRE-INSTALLED FOUR (4) SET-SCREWS IN THE SHROUD, WHICH TIGHTEN AGAINST THE BARREL.

NOTE: It is easier to ID certain parts during the Top Rail installation if you have the Hi-Point Owner Manual open to the pages showing the gun assembly diagrams. If you no longer have the original manual, it can usually be downloaded from the internet and/or viewed directly on the Hi-Point website.

ALWAYS BEGIN ANY INSTALLATION WITH THE GUN COMPLETELY UNLOADED.

**NOTE**: IF YOUR CARBINE HAS THE FACTORY PLASTIC RAIL INSTALLED BENEATH THE BARREL, IT WILL FIRST NEED TO BE ROMOVED.

TO REMOVE THE FACTORY RAIL LOCATED BENEATH THE BARREL:

1. REMOVE MAGAZINE CLIP FROM GUN.
2. WITH THE CHAMBER CLOSED AND THE GUN **UNLOADED**, COMPLETELY REMOVE THE CHARGING HANDLE ALONG WITH ITS MOUNTING BOLT. ALSO, LOOSEN AND/OR REMOVE TOP RAIL AND/OR ANY ACCESSORIES THAT MAY INHIBIT REMOVAL OF THE METAL RECEIVER SHROUD.
3. REMOVE FRONT IRON SIGHT FROM BARREL.
4. ON THE LEFT SIDE OF THE GUN, LOOSEN AND/OR REMOVE THE FASTENERS THAT SECURE THE METAL RECEIVER COVER SHROUD TO THE GUN.
5. LIFT AND REMOVE THE METAL RECEIVER COVER FROM THE GUN.
6. REMOVE STOCK CLIPS AND RECEIVER CLIP.
7. REMOVE PLASTIC FOREND COVER AT THE FRONT OF THE STOCK BY SLIDING IT FORWARD. (IT IS A VERY SNUG FIT AND MAY REQUIRE SOME EFFORT TO SLIDE IT FORWARD)
8. LIFT AND REMOVE ENTIRE FIRING ASSEMBLY AND BARREL FROM STOCK.
9. REMOVE THE FARTHEST FORWARD STOCK BOLT FROM SIDE OF PLASTIC FORE-END (NO NEED TO REMOVE ANY OF THE OTHER BOLTS.)
10. REMOVE PLASTIC BARREL RAIL AND THEN RE-INSTALL THE SCREW BACK INTO THE PLASTIC STOCK BUT DO NOT FULLY TIGHTEN YET.
11. REASSEMBLE GUN IN REVERSE ORDER OF DISASSEMBLY.
12. CHECK EVERYTHING FOR PROPER OPERATION AND THAT YOU DID NOT FORGET TO REPLACE ANY OF THE ITEMS THAT YOU REMOVED DURING THE DISASSEMBLY PROCESS.
13. INSTALL THE NEW INTEGRATED SHROUD ONTO THE BARREL AND PUSH IT INTO POSITION WITHIN THE SQUARE OPENING OF THE STOCK.
14. FINISH RE-TIGHTENING STOCK SCREW. TIGHTEN THE 4 SET-SCREWS WITHIN THE SHROUD.
15. THAT’S IT, YOU’RE DONE.
16. Got questions or are uncertain of the installation process, please call us at 973-786-4004 and we can guide you over the phone.