

**INSTALLATION INSTRUCTIONS**

**Magazine Release Button for 9mm w/ATI Stock**

1. It is easier to identify certain parts during the installation if you have the Hi-Point Owner’s Manual open to the pages showing the gun assembly diagrams. If you no longer have the original manual, it can be downloaded and/or viewed directly on the Hi-Point website, or you can email sales@longshotmfg.com for a PDF copy.
2. REMOVE MAGAZINE CLIP FROM GUN.
3. WITH THE CHAMBER CLOSED AND THE GUN **UNLOADED**, COMPLETELY REMOVE THE CHARGING HANDLE ALONG WITH ITS MOUNTING BOLT. ALSO, LOOSEN AND/OR REMOVE TOP RAIL AND/OR ANY ACCESSORIES THAT MAY INHIBIT REMOVAL OF THE METAL RECEIVER SHROUD.
4. REMOVE PLASTIC FOREND COVER AT THE FRONT OF THE STOCK.
5. ON ONE SIDE OF THE GUN, LOOSEN AND REMOVE THE FASTENERS THAT SECURE THE METAL RECEIVER COVER SHROUD TO THE GUN.
6. LIFT AND REMOVE THE METAL RECEIVER COVER FROM THE GUN.
7. REMOVE STOCK CLIPS AND RECEIVER CLIP.
8. REMOVE THE BARREL MOUNT/SUPPORT SCREWS AND BRACKET THAT SECURE THE BARREL AT THE FRONT AREA OF THE STOCK .
9. LIFT AND REMOVE ENTIRE FIRING ASSEMBLY AND BARREL FROM STOCK.
10. IF NEED BE, REMOVE THE MAGAZINE RELEASE SIDEPLATE COVER TO ALLOW EASIER ACCESS TO THE RELEASE LEVER AND SPRING. (TAKE CARE NOT TO LOSE THE SMALL SPRING WHEN REMOVING CATCH. YOU MAY HAVE TO REMOVE MAGAZINE CATCH CAP BY PUSHING THRU TO INSIDE OF STOCK)
11. PLACE SUPPLIED NEW O-RING ONTO MAGAZINE CATCH PIN DIAMETER AND SLIDE IT TOWARD THE CATCH LEVER.
12. CAREFULLY REINSTALL MAGAZINE CATCH AND SPRING BACK INTO PLACE WITHIN THE STOCK WHILE KEEPING THE O-RING LOCATED ON THE PIN DIAMETER.
13. RE-INSTALL THE RELEASE PIN COVER PLATE .REINSTALL THE HANDLE SUPPORT SCREWS AND STOCK RETAINER CLIP AT THIS TIME.
14. INSERT SUPPLIED NEW OVERSIZED MAG RELEASE BUTTON INTO PLACE AND ONTO CATCH PIN DAIMETER.
15. WHILE USING ONE HAND TO PUSH ON THE MAG RELEASE BUTTON, REACH INTO THE STOCK WITH FINGERS OF YOUR OTHER HAND AND CAREFULLY ROLL THE O-RING ONTO THE SHAFT OF THE RELEASE BUTTON UNTIL IT IS CAPTURED IN THE MACHINED O-RING GROOVE.
16. TEMPORARILY RETURN FIRING ASSEMBLY AND BARREL BACK INTO PLACE WITHIN THE STOCK. RETURN MAGAZINE INTO PLACE WITHIN THE PISTOL GRIP AND CHECK FOR PROPER RELEASE ACTION WITH THE NEW RELEASE BUTTON. USE THE SUPPLIED HEX KEY TO ADJUST THE ADJUTMENT SET-SCREW IN THE CENTER OF THE MAG RELEASE BUTTON FOR PROPER RELELEASE AND MAG RETENTION IF RELEASE FUNCTIONS PROPERLY, REASSEMBLE GUN IN REVERSE ORDER OF DISASSEMBLY. FULL REASSEMBLY WITH ALL BOLTS TIGHTENED WILL PROVIDE BEST DETERMINATION OF RELEASE FUNCTIONS AS IT IS SUPPOSED TO. (SOME MAGAZINES MAY REQUIRE SLIGHT POLISHING OF CONTACT AREAS FOR SMOOTHEST RELEASE. )
17. CHECK EVERYTHING FOR PROPER OPERATION AND THAT YOU DID NOT FORGET TO REPLACE ANY OF THE ITEMS THAT YOU REMOVED DURING THE DISASSEMBLY PROCESS. FINE ADJUST FOR SMOOTHEST RELEASE FUNCTION BY DOING FINAL ADJUSTMENT OF THE SET SCREW IN THE CENTER OF THE MAG BUTTON.
18. LASTLY, THIS IS THE MOST IMPORTANT STEP….PLEASE EMAIL US WITH YOUR COMMENTS ABOUT OUR PRODUCT AND THE INSTALLATION PROCESS AND THE EASE OF USING OUR INSTALLATION INSTRUCTIONS.