ASSEMBLY INSTRUCTION – BASE CABINET (CLIP SYSTEM)

|  |  |
| --- | --- |
|  | * Lay door front on face with clips facing up * Tip: loosen flat clips a little to allow easier fit |
|  | * Insert side panel into clips and snugly into groove |
|  | * Insert other side panel in the same way |
|  | * Tighten screws in clips |

|  |  |
| --- | --- |
|  | * Slide bottom into grooves |
|  | * Attach back into clips |
|  | * Stand cabinet upright and tighten all screws in clips |
|  | * Attach toe kick into clips and tighten |
| Brackets and Corner Supports |  |