|  |  |  |
| --- | --- | --- |
| **Developed By** | **Reviewed By** | **Updated** |
| Russell EisenhauerDwayne Cunningham | WAGPI JOHS Committee |  |

|  |  |  |
| --- | --- | --- |
| **Equipment Required** | **Material Required** | **Personal Protective Equipment** |
| Tractor / Backhoe |  | Steel toe footwear |
| Punt |  | Eye protection |
| Winch |  | Life jacket |
| Manpower |  | Gloves |
| Wrenches |  | Hard hat |
| Hammer |  |  |
| Pry Bar |  |  |
| Chains / Straps |  |  |
|  |  |  |

**Job Steps**

1. Wear life jacket

2. Check docks/wharves for winter damage

3. Check bolts/rope/pins/moorings to hook up dock

4. Get manpower in place to move dock. Or tractor/backhoe if too large/heavy

5. Put dock in water

6. Pull/paddle/tow dock to location

7. Line up dock and put in pins/bolts

8. Pin/bolt/secure wharf/dock for season

9. Gather tools, equipment

10. Check with customer before leaving site for satisfaction.