|  |  |  |
| --- | --- | --- |
| **Developed By** | **Reviewed By** | **Updated** |
| Michelle Lohnes | WAGPI JOHS Committee |  |

|  |  |  |
| --- | --- | --- |
| **Equipment Required** | **Material Required** | **Personal Protective Equipment** |
| Slinger | Aggregrate | Steel toe footwear |
|  |  | Safety Vest |
|  |  | Hard Hat |
|  |  | Gloves |
|  |  | Eye Protection |

**Job Steps**

1. Park on firm level bottom.
2. Set park brake.
3. Check job site for obstruction, over head wires etc.
4. Ensure area around slinger in clear of workmen.
5. Extend stick conveyor.
6. Proceed to unload.
7. Never leave slinger unattended with conveyor running.
8. Fold conveyor back in.
9. Check for stones that may fall off while driving on the highway.