Drainable Leg Tanks

When complete drainage is necessary, these are the tanks of choice. They are designed primarily for use on fertilizer and chemical nurse trailers. All Norwesco drainable leg tanks require full length bottom support as well as support bands.

[View Fitting Installation Guide for Drainable Leg Tanks](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/FITTING%20INSTALLATION%20GUIDE%20FOR%20DRAINABLE%20LEG%20TANKS.pdf)

|  |
| --- |
| **Drainable Leg Tanks** |
| **Gallon Capacity** | **Width** | **Overall Height** | **Length** | **Fill Opening** | **Outlet/Drain Specification** | **Premium Weight Part No. White** | **Avail** | **Heavy Weight Part No. Blue** | **Avail** |
| 710 (horizontal) | 47" | 57" | 104" | 16"-(63485) | 2"-(63683) \* | [40655](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/710%20Gallon%20Horizontal%20Drainable%20Tank.pdf) | F | [40657](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/710%20Gallon%20Horizontal%20Drainable%20Tank.pdf) | C |
| 1010 (horizontal) | 47" | 58" | 140" | 16"-(63485) | 2"-(63683) \* | [40393](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/1010%20Gallon%20Horizontal%20Drainable%20Tank.pdf) | B,C,E,L | [40395](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/1010%20Gallon%20Horizontal%20Drainable%20Tank.pdf) | B,C,E,L |
| 1310 (horizontal) | 66" | 75" | 99" | 16"-(63485) | N/A | [41871](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/1310%20Gallon%20Horizontal%20Drainable%20Tank.pdf) | B | [41872](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/1310%20Gallon%20Horizontal%20Drainable%20Tank.pdf) | B |
| 1315 (elliptical) | 66" | 60" | 126" | 16"-(63485) | N/A | [42925](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/1315%20Gallon%20Elliptical%20Drainable%20Tank.pdf) | B,F | [42926](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/1315%20Gallon%20Elliptical%20Drainable%20Tank.pdf) | B,C,F |
| 1610 (elliptical) | 69" | 63" | 140" | 16"-(63485) | N/A | [40806](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/1610%20Gallon%20Elliptical%20Drainable%20Tank.pdf) | B,C,E,F | [40808](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/1610%20Gallon%20Elliptical%20Drainable%20Tank.pdf) | B,C,E,F |
| 2010 (elliptical) | 69" | 74" | 140" | 16"-(63485) | N/A | [43651](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/2010%20Gallon%20Elliptcial%20Drainable%20Tank.pdf) | B,E | [43652](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/2010%20Gallon%20Elliptcial%20Drainable%20Tank.pdf) | B,E,F |
| 2610 (elliptical) | 90" | 79" | 140" | 16"\*-(62532) | N/A | [41382](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/2610%20Gallon%20Elliptical%20Drainable%20Tank.pdf) | B,C | [41383](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/2610%20Gallon%20Elliptical%20Drainable%20Tank.pdf) | B,C,F |
| 3210 (elliptical) | 92" | 75" | 178" | 16"\*-(62532) | N/A | [40822](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/3210%20Gallon%20Elliptical%20Drainable%20Tank.pdf) | B,C,E | [40824](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/3210%20Gallon%20Elliptical%20Drainable%20Tank.pdf) | B,C,E |
| \*Fitting is loose, not installed |
|  Drainable Leg Tanks REQUIRE FULL LENGTH SUPPORT AND SUPPORT BANDS. |

Drainable Leg Tank Bands

Norwesco bands are custom fabricated to support the Norwesco tanks and are galvanized or powder coated for added corrosion protection. Whether using the tank in a stationary position or for transport, bands are necessary to ensure that the tank retains its shape and integrity.

|  |
| --- |
| **Drainable Leg Tank Bands** |
| **Tank Size (Gallon)** | **A** | **B** | **C** | **Color of band foot** | **No. of Bands** | **Part No.** |  |  |
| 710¤ | 46 1/4" | 45" | 51" | Green | 3 required | [60584 short](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/710%20Gallon-1010%20Gallon%20%28Short%29%20Drainable%20Leg%20Tank%20Band%20PN.pdf) |  |  |
| \*1010¤ | 46 1/4" | 45" | 51" | Green | 2 required | [60584 short](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/710%20Gallon-1010%20Gallon%20%28Short%29%20Drainable%20Leg%20Tank%20Band%20PN.pdf) |  |  |
| \*1010¤ | 48" | 45" | 51" | Red | 2 required | [60585 long](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/1010%20Gallon%20%28Long%29%29%20Drainable%20Leg%20Tank%20Band%20PN.pdf) |  |  |
| 1310 | 64" | 64" | 70" | White | 3 required | [63282](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/1310%20Gallon%20Drainable-1325%20Gallon%20Horizontal%20Tank%20Band%20PN.pdf) |  |  |
| 1315 | 49 3/4" | 63 1/2" | 69 1/2" | Blue | 3 required | [63642](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/1335%20Gallon%20Elliptical%20Leg%20Tank-1315%20Gallon%20Drainable%20Leg%20Tank%20Band%20PN.pdf) |  |  |
| 1610 | 49" | 66" | 72" | Orange | 4 required | [62434](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/1610%20Gallon%20Drainable%20Leg%20Tank%20Band%20PN.pdf) |  |  |
| 2010 | 59" | 66" | 72" | Galvanized | 4 required | [63846](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/2010%20Gallon%20Drainable%20Leg%20Tank%20Band%20PN.pdf) |  |  |
| \*2610 | 58" | 87 1/2" | 91 7/8" | Entire band painted Powder Gray.There are 2 notches cut into the foot. | 2 required | [63044 short](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/2610%20Gallon%20Drainable%20Leg%20Tank%20Short%20Band%20PN.pdf) |  |  |
| \*2610 | 62" | 87 1/2" | 91 7/8" | Entire band painted Powder Gray.There are 2 notches cut into the foot. This band also has a welded ladder bracket on top of the band. | 2 required | [63045 long](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/2610%20Gallon%20Drainable%20Leg%20Tank%20Long%20Band%20PN.pdf) |  |  |
| \*3210 | 56" | 89 1/2" | 92 3/4" | Entire band painted Powder Gray.There are 3 notches cut into the foot. | 2 required | [62347 short](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/3210%20Gallon%20Drainable%20Leg%20Tank%20Short%20Band%20PN.pdf) |  |  |
| \*3210 | 60" | 89 1/2" | 92 3/4" | Entire band painted Powder Gray.There are 3 notches cut into the foot.This band also has a welded ladder bracket on top of the band. | 2 required | [62348 long](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/3210%20Gallon%20Drainable%20Leg%20Tank%20Long%20Band%20PN.pdf) |  |  |
| \*2 short and 2 long bands are required for 1 tank.¤May ship UPS |  |  |

|  |
| --- |
| **Ladder** |
| **Description** | **Tank Size (Gallon)** | **Part No.** |  |  |  |  |  |  |  |
| Ladder-powder coated (optional) | 2610 & 3210 | [63047](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/2610_3210%20Gallon%20Drainable%20Leg%20Tank%20Ladder%20PN.pdf) |  |  |  |  |  |  |  |