
Horizontal Leg Tanks

With the broadest leg tank line available, Norwesco manufactures a size that will fit your needs. Used primarily for transport and nursing applications, Norwesco's leg tanks feature molded-in legs that act as "baffles" to reduce sloshing.

[View Fitting Installation Guide for Horizontal Leg Tanks](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/FITTING%20INSTALLATION%20GUIDE%20FOR%20HORIZONTAL%20LEG%20TANKS.pdf)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Horizontal Leg Tanks** | | | | | | | | | |
| **Gallon Capacity** | **Diameter** | **Overall Height** | **Length** | **Fill Opening** | **Outlet/Drain Specification** | **Premium Weight Part No. White** | **Avail** | **Heavy Weight Part No. Blue** | **Avail** |
| 35¤ | 20" | 23" | 29" | 5"-(63484) | 3/4"-(60401) | [45223](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/35%20Gallon%20Horizontal%20Tank.pdf) | A | NA | - |
| 55¤ | 23" | 26" | 34" | 5"-(63484) | 3/4"-(60401) | [41873](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/55%20Gallon%20Horizontal%20Leg%20Tank.pdf) | A | NA | - |
| 65¤ | 23" | 26" | 43" | 5"-(63484) | 3/4"-(60401) | [45191](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/65%20Gallon%20Horizontal%20Tank.pdf) | A | NA | - |
| 125 | 32" | 35" | 41" | 8"-(63480) | 2"-(63481) 2" siphon (60335) | [40298](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/125%20Gallon%20Horizontal%20Leg%20Tank.pdf) [40298 GA-OK-TX(T)](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/125%20Gallon%20Leg%20Tank%20Side%20Port%20GA-OK-TX.pdf) | B,C,D,E,F,G,H,I,L,P,T | NA | - |
| 225 | 38" | 41" | 49" | 8"-(63480) | 2"-(63481) 2" siphon (60335) | [40299](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/225%20Gallon%20Horizontal%20Leg%20Tank.pdf) [40299-OK-NY-TX(P&T)](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/225%20Gallon%20Horizontal%20Leg%20Tank%20-OK-NY-TX.pdf) | B,C,D,E,F,G,H,I,L,P,T | NA | - |
| 325 | 38" | 43" | 68" | 16"-(63485) | 2"-(63481) 2" siphon (60335) | [40217](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/325%20Gallon%20Horizontal%20Leg%20Tank.pdf) | A | NA | - |
| 425 | 49" | 54" | 60" | 16"-(63485) | 2"-(63481) 2" siphon (60335) | [42016](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/425%20Gallon%20Horizontal%20Tank.pdf) | B,C,D,F,T | N/A | - |
| 525\* | 49" | 54" | 71" | 16"-(63485) | 2"-(63481) 2" siphon (60335) | [40181](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/525%20Gallon%20Horizontal%20Leg%20Tank.pdf) [40181-GA-TX-OK](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/525%20Gallon%20Horizontal%20Leg%20Tank%20-GA-TX-OK.pdf) | B,C,D,E,F,G,H,L,T | [40193](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/525%20Gallon%20Horizontal%20Leg%20Tank.pdf) [40193-GA-TX-OK](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/525%20Gallon%20Horizontal%20Leg%20Tank%20-GA-TX-OK.pdf) | B,C,E,F,G,H,L,T |
| 725\*\* | 49" | 54" | 101" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [40180](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/725%20Gallon%20Horizontal%20Leg%20Tank.pdf) [40180-GA-OH-NY](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/725%20Gallon%20Horizontal%20Leg%20Tank%20OH%20GA%20NY.pdf) | C,D,E,F,G,T | [40194](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/725%20Gallon%20Horizontal%20Leg%20Tank.pdf) [40194-GA-OH](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/725%20Gallon%20Horizontal%20Leg%20Tank%20OH%20GA%20NY.pdf) | C,D,E,F,T |
| 925\*\* | 62" | 65" | 80" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [45209](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/925%20Gallon%20Horizontal%20Leg%20Tank.pdf) | C | NA | - |
| 925 w/sump\*\* | 62" | 69" | 80" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [45210](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/925%20Gallon%20Horizontal%20Leg%20Tank%20w%20Sump.pdf) | C | NA | - |
| 1025\*\* | 49" | 54" | 139" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [40089](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1025%20Gallon%20Horizontal%20Leg%20Tank.pdf) [40089-GA-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1025%20Gallon%20Horizontal%20Leg%20Tank%20GA%20TX.pdf) | B,C,D,E,F,G,H,L,T | [40131](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1025%20Gallon%20Horizontal%20Leg%20Tank.pdf) [40131-GA-TX](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1025%20Gallon%20Horizontal%20Leg%20Tank%20GA%20TX.pdf) | B,C,D,E,F,G,H,L,T |
| 1325\*\* | 66" | 70" | 99" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [41875](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1325%20Gallon%20Horizontal%20Leg%20Tank.pdf) | C | [41877](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1325%20Gallon%20Horizontal%20Leg%20Tank.pdf) | C |
| 1625\*\* | 63" | 68" | 139" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [40026](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1625%20Gallon%20Horizontal%20Leg%20Tank.pdf) | C | [40133](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1625%20Gallon%20Horizontal%20Leg%20Tank.pdf) | C |
| 1800\*\*- 2CPT § | 62" | 68" | 146" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [42990-UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1800%20Gallon%202-Compartment%20Leg%20Tank.pdf) [42990-TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1800%20Gallon%202-Compartment%20Leg%20Tank%20Component.pdf) [42994-DONUT](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1800%20Gallon%202-Compartment%20Tank%20Donut%20PN.pdf) [63653-BAR](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1800%20Gallon%202-Compartment%20Tank%20Tie%20Strap%20PN.pdf) | C | - | - |
| 1800\*\* w/sump, 2CPT § | 62" | 72" | 146" | 16"-(63485) | 2"-(63683) 2" siphon (60335) | [42992-UNIT](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1800%20Gallon%202-Compartment%20Leg%20Tank%20with%20Sump.pdf) [42992-TANK](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1800%20Gallon%202-Compartment%20Leg%20Tank%20Component%20with%20Sump.pdf) [42994-DONUT](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1800%20Gallon%202-Compartment%20Tank%20Donut%20PN.pdf) [63653-BAR](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/1800%20Gallon%202-Compartment%20Tank%20Tie%20Strap%20PN.pdf) | C | - | - |
| 3725\*\* | 92" | 97" | 145" | 16"-(63485) | 3"-(62299) 2" reducer (60330) 3" siphon (60327) | [44047](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/3725%20Horizontal%20Leg%20Tank.pdf) | B,E,T | [44049](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/3725%20Horizontal%20Leg%20Tank.pdf) | B,E,T |
| 5025\*\* | 92" | 96" | 190" | 16" hinged-(62532) | 3"-(62299) 2" reducer (60330) 3" siphon (60327) | [41879](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/5025%20Gallon%20Horizontal%20Leg%20Tank.pdf) | B,C,E,L | [41881](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/5025%20Gallon%20Horizontal%20Leg%20Tank.pdf) | B,C,E,L |
| 6025\*\* w/baffles | 99" | 103" | 193" | 22" hinged-(63874) | 3"-(62299) 2" reducer (60330) 3" siphon (60327) | [44314](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/6025%20Horizontal%20Leg%20Tank.pdf) | B,C,E | [44316](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/6025%20Horizontal%20Leg%20Tank.pdf) | B,C,E |

\*Requires full length support.  
\*\*Require full length support and bands.  
 § Tank consists of 2-900 gallon tanks, each with a fitting installed, and a cylindrical 'donut' that with the connecting bar listed below, holds the two tanks together but does not plumb them together.

Horizontal Leg Tank Bands

Norwesco bands are custom fabricated to support the Norwesco tanks and are galvanized for added corrosion protection. Whether using the tank in a stationary position or for transport, bands are necessary to ensure that the tank retains its shape and integrity.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Horizontal Leg Tank Bands** | | | | | | |
| **Tank Size (Gallon)** | **A** | **B** | **C** | **Color of band foot** | **No. of Bands** | **Part No.** |
| 35¤ | 18 1/2" | 18 1/2" | 21 3/8" | Galvanized 1" EMT | 2 optional | [60520](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/35%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |
| 55¤ | 22" | 22" | 26 1/2" | Galvanized 1" EMT | 2 optional | [61745](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/55-65%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |
| 65¤ | 22" | 22" | 26 1/2" | Galvanized 1" EMT | 2 optional | [61745](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/55-65%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |
| 125¤ | 30 3/4" | 30 1/2" | 35" | Galvanized | 2 optional | [61744](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/125%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |
| 225¤ | 36 1/2" | 36" | 42" | Galvanized | 2 optional | [60478](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/225-325-330%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |
| 325¤ | 36 1/2" | 36" | 42" | Galvanized | 2 optional | [60478](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/225-325-330%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |
| 425 | 47 3/4" | 46 1/4" | 52 1/4" | Entire band painted gray GA-OH-NY  Galvanized all other plants | 2 optional | [60057](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/425-525-725-1025%20Gal%20Horiz%20Leg%20Tank%20Band%20PN.pdf) |
| 525 | 47 3/4" | 46 1/4" | 52 1/4" | Entire band painted gray GA-OH-NY Galvanized all other plants | 2 optional | [60057](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/425-525-725-1025%20Gal%20Horiz%20Leg%20Tank%20Band%20PN.pdf) |
| 725 | 47 3/4" | 46 1/4" | 52 1/4" | Entire band painted gray GA-OH-NY Galvanized all other plants | 3 required | [60057](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/425-525-725-1025%20Gal%20Horiz%20Leg%20Tank%20Band%20PN.pdf) |
| 925 | 61" | 60" | 66" | Galvanized-small lime green flat welded on the top. | 2 required | [62852](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/925-1800%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |
| 1025 | 47 3/4" | 46 1/4" | 52 1/4" | Entire band painted gray GA-OH-NY Galvanized all other plants | 4 required | [60057](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/425-525-725-1025%20Gal%20Horiz%20Leg%20Tank%20Band%20PN.pdf) |
| 1325 | 64" | 64" | 70" | White | 3 required | [63282](https://www.norwesco.com/_site_components/uploads/pdfs/Drainable%20Leg/Drainable%20Leg%20Steel/1310%20Gallon%20Drainable-1325%20Gallon%20Horizontal%20Tank%20Band%20PN.pdf) |
| 1625 | 61" | 60 3/4" | 67 1/4" | Galvanized | 4 required | [60079](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/1625%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |
| 1800 † | 61" | 60" | 66" | Galvanized-small lime green flat welded on the top. | 4 required | [62852](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/925-1800%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |
| 3725 | 89 3/4" | 89 1/2" | 93 7/8" | Galvanized | 4 required | [63284](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/3725-5025%20Gallon%20Horizontal%20Tank%20Band%20PN.pdf) |
| 5025 | 89 3/4" | 89 1/2" | 93 7/8" | Galvanized | 5 required | [63284](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/3725-5025%20Gallon%20Horizontal%20Tank%20Band%20PN.pdf) |
| 6025 | 96" | 96 1/4" | 101" | Dark Blue | 5 required | [64085](https://www.norwesco.com/_site_components/uploads/pdfs/Horizontal%20Leg/Horizontal%20Leg%20Steel/6025%20Gallon%20Horizontal%20Leg%20Tank%20Band%20PN.pdf) |

† Tank requires one connecting bar, part #63653  
EMT=Electrical Metallic Tubing