Pickup Truck Tanks

Designed to fit full-size, American-made pickups, the 325 and 425 sizes have low profiles for better rear vision. They feature fill openings offset to the side of the tank for safety and easy access. A tough circular design adds strength. The 210 gallon tank fits both "mini" pickups and full-size models. Depending on which way the tank is turned, the bottom width can be either 39" or 48".

|  |
| --- |
| **Pickup Truck Tanks** |
| **Gallon Capacity** | **Top Width or Diameter** | **Bottom Width or Diameter** | **Overall Height** | **Fill Opening** | **Outlet/Drain Specification** | **Premium Weight Part No. White** | **Avail** |  |  |
| 210 | 60"/51" | 48"/39" | 29" | 8"-(63480) | 2"-(63481) 2" siphon (60335) | [40300](https://www.norwesco.com/_site_components/uploads/pdfs/Pickup/210%20Gallon%20Pickup%20Tank.pdf) | B,C,D,E,F,G,H,I,L,P,T |  |  |
| 305 | 60" | 48" | 30" | 8"-(63480) | 2"-(63481) 2" siphon (60335) | [44808](https://www.norwesco.com/_site_components/uploads/pdfs/Pickup/305%20Gallon%20Pickup%20Tank.pdf) | C,E,I |  |  |
| 325 | 62" | 49" | 33" | 8"-(63480) | 2"-(63481) 2" siphon (60335) | [40160](https://www.norwesco.com/_site_components/uploads/pdfs/Pickup/325%20Gallon%20Pickup%20Tank.pdf) | B,C,D,E,F,G,H,I,L,P,T |  |  |
| 425 | 65" | 49" | 39" | 8"-(63480) | 2"-(63481) 2" siphon (60335) | [40102](https://www.norwesco.com/_site_components/uploads/pdfs/Pickup/425%20Gallon%20Pickup%20Tank.pdf) | B,C,D,E,F,G,H,I,L,P,T |  |  |