Chemical Injection Tank Systems

Our chemical injection tank system is designed for applications in the oil and gas industry.  The package includes a leg tank, stand, and enclosed containment basin.  The enclosed containment basins have a pump mount, a 2" and a 3" female threaded connection for additional items such as solar panels.

|  |
| --- |
| **Chemical Injection Tank Systems** |
| **Part #** | **Description** | **Diameter/Width** | **Height** | **Length** | **FillOpening** | **Avail** |  |  |  |  |
| [44099](https://www.norwesco.com/_site_components/uploads/pdfs/Chemical%20Injection%20System/65%20Injection%20System%20Assy%20PN.pdf) | 65 Chemical Injection System (tank, stand, basin)65 Leg TankStand for 65 Leg TankContainment Basin - 95 Gallon | 23"23"36" | 26"32"11" | 43"33 1/2"61" | 5"-(63484) | E,I |  |  |  |  |
| [63880](https://www.norwesco.com/_site_components/uploads/pdfs/Chemical%20Injection%20System/125%20Injection%20System%20Assy%20PN.pdf) | 125 Chemical Injection System (tank, stand, basin)125 Leg TankStand for 125 Leg TankContainment Basin - 165 Gallon | 32"32"45" | 35 1/2"32"14 1/2" | 43 1/2"30 1/4"64" | 6" | E,M\* |  |  |  |  |
| [63885](https://www.norwesco.com/_site_components/uploads/pdfs/Chemical%20Injection%20System/225%20Injection%20System%20Assy%20PN.pdf) | 225 Chemical Injection System (tank, stand, basin)225 Leg TankStand for 225 Leg TankContainment Basin - 300 Gallon | 38"38"54" | 41 1/2"30"15 1/2" | 52"34 1/2"89" | 6" | E,M\* |  |  |  |  |
| [63890](https://www.norwesco.com/_site_components/uploads/pdfs/Chemical%20Injection%20System/335%20Injection%20System%20Assy%20PN.pdf) | 335 Chemical Injection System (tank, stand, basin)335 Leg TankStand for 335 Leg TankContainment Basin - 380 Gallon | 44"38"54" | 49"30"19 1/2" | 56"34 1/2"80" | 6" | E,M\* |  |  |  |  |