

Loaf Tanks

The loaf tanks are designed for a variety of applications. Its rectangular shape allows for placement within pickup beds or it may be mounted on various equipment trailers for use as a mobile water supply. This line of tanks may also be used in a variety of stationary storage applications.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Loaf Tanks** | | | | | | | |
| **Gallon Capacity** | **Width** | **Overall Height** | **Length** | **Outlet/Drain Specification** | **Fill Opening** | **Premium Weight Part No. White** | **Avail** |
| 50¤ | 20" | 16" | 48" | N/A | 8"-(63480) | [44962](https://www.norwesco.com/_site_components/uploads/pdfs/Loaf/50%20Gallon%20x%2048%20L%20Loaf%20Tank.pdf) | C,I,L,X |
| 50¤ | 27" | 17" | 41" | N/A | 8"-(63480) | [43610](https://www.norwesco.com/_site_components/uploads/pdfs/Loaf/50%20Gallon%20Loaf%20Tank.pdf) | C,I,L,X |
| 100¤ | 20" | 32" | 48" | N/A | 8"-(63480) | [44963](https://www.norwesco.com/_site_components/uploads/pdfs/Loaf/100%20Gallon%20x%2048%20L%20Loaf%20Tank.pdf) | C,I,L,X |
| 100¤ | 27" | 30" | 41" | N/A | 8"-(63480) | [43611](https://www.norwesco.com/_site_components/uploads/pdfs/Loaf/100%20Gallon%20Loaf%20Tank.pdf) | C,I,L,X |
| 200 | 36" | 29" | 48" | N/A | 8"-(63480) | [43612](https://www.norwesco.com/_site_components/uploads/pdfs/Loaf/200%20Gallon%20x%2036%20W%20Loaf%20Tank.pdf) | C,I,L,X |
| 200 | 40" | 31" | 48" | N/A | 8"-(63480) | [45380](https://www.norwesco.com/_site_components/uploads/pdfs/Loaf/200%20Gallon%20x%2040%20W%20Loaf%20Tank.pdf) | C,I,L,X |
| 300 | 42" | 30" | 63" | N/A | 8"-(63480) | [43613](https://www.norwesco.com/_site_components/uploads/pdfs/Loaf/300%20Gallon%20Loaf%20Tank.pdf) | C,I,L,X |
| 500 | 48" | 31" | 92" | N/A | 8"-(63480) | [43843](https://www.norwesco.com/_site_components/uploads/pdfs/Loaf/500%20Gallon%20Loaf%20Tank.pdf) | C,I,L,X |
| 1050 | 60" | 49" | 96" | N/A | 8"-(63480) | [44936](https://www.norwesco.com/_site_components/uploads/pdfs/Loaf/1050%20Gallon%20Loaf%20Tank.pdf) | B,E,F,L |