|  |
| --- |
| 1. Air Brake System
 |
| Defect(s)* Audible air leak
* Slow air pressure build up rate
 | Major Defect(s)* Pushrod stroke of any brake exceeds the adjustment limit
* Air loss rate exceeds prescribed limit
* Inoperative towing vehicle(tractor) protection system
* Low air warning system fails, or system is activated
* Inoperative service, parking, or emergency brake
 |
| 1. Cab
 |
| Defect(s)* Occupant compartment door fails to open
 | Major Defect(s)* Any cab or sleeper door fails to close securely
 |
| 1. Cargo Securement
 |
| Defect(s)Insecure or improper load covering (e.g. wrong type or flapping in the wind. | Major Defect(s)* Insecure cargo
* Absence, failure, malfunction or deterioration of required cargo securement device or load covering
 |
| 1. Coupling Devices
 |
| Defect(s) * Coupler or mounting has loose or missing fastener
 | Major Defect(s)* Coupler is insecure, or movement exceeds prescribed limit
* Coupling or locking mechanism is damaged or fails to lock
* Defective, incorrect or missing safety chain/cable
 |
| 1. Dangerous Goods
 |
| Defects(s) | Major Defect(s)* Dangerous Goods requirements not met
 |
| 1. Driver Controls
 |
| Defect(s)* Accelerator pedal, clutch, gauges, audible and visual indicators or instruments fail to function properly
 | Major Defect(s) |
| 1. Driver Seat
 |
| Defect(s)* Seat is damaged or fails to remain in set position
 | Major Defect(s)* Seatbelt or tether belt is insecure, missing or malfunctions
 |
| 1. Electric Brake System
 |
| Defect(s)* Loose or insecure wiring or electrical connection
 | Major Defect(s)* Inoperative breakaway device
* Inoperative brake
 |
| 1. Emergency Equipment & Safety Devices
 |
| Defect(s)* Emergency equipment is missing, damaged or defective
 | Major Defect(s) |
| 1. Exhaust System
 |
| Defect(s)* Exhaust leak
 | Major Defect(s)* Leak that causes exhaust gas to enter the occupant compartment
 |
| 1. Frame and Cargo Body
 |
| Defect(s)* Damaged frame or cargo body
 | Major Defect(s)* Visibly shifted, cracked, collapsing or sagging frame member(s).
 |
| 1. Fuel System
 |
| Defect(s)* Missing fuel tank cap
 | Major Defect(s)* Insecure fuel tank
* Dripping fuel leak
 |
| 1. General
 |
|  | Major Defect(s)* Serious damage or deterioration that is noticeable and may affect the vehicle’s safe operation
 |
| 1. Glass and Mirrors
 |
| Defect(s)* Required mirror or window glass fails to provide the required view to the driver as a result of being cracked, broken, damaged, missing or maladjusted
* Required mirror or glass has broken or damaged attachments onto vehicle body
 | Major Defect(s) |
| 1. Heater/Defroster
 |
| Defect(s)* Control or system failure
 | Major Defect(s)* Defroster fails to provide unobstructed view through the windshield
 |
| 1. Horn
 |
| Defect(s)* Vehicle has no operative horn
 | Major Defect(s) |
| 1. Hydraulic Brake System
 |
| Defect(s)* Brake fluid level is below indicated minimum level
 | Major Defect(s)* Parking brake is inoperative
* Brake boost or power assist is inoperative
* Brake fluid leak
* Brake pedal fade or insufficient brake pedal reserve
* Activated (other than ABS) warning device
* Brake fluid reservoir is less than ¼ full
 |
| 1. Lamps and Reflectors
 |
| Defect(s)* Required lamp does not function as intended
* Required reflector is missing or partially missing
 | Major Defect(s)When Lamps are required:* Failure of both low-beam headlamps
* Failure of both rearmost tail lamps

At all times:* Failure of a rearmost turn-indicator lamp
* Failure of both rearmost brake lamps
 |
| 1. Steering
 |
| Defect(s)* Steering wheel lash (free-play) is greater than normal
 | Major Defect(s)* Steering wheel is insecure, or does not respond normally
* Steering wheel lash (free-play) exceeds required limit
 |
| 1. Suspension System
 |
| Minor Defect(s)* Air leak in air suspension system
* Broken spring leaf
* Suspension fastener is loose, missing or broken
 | Major Defect(s)* Damaged (patched, cut, bruised, cracked to braid, mounted insecurely) or deflated air bag
* Cracked or broken main spring leaf or more than one broken spring leaf
* Part of spring leaf or suspension is missing, shifted out of place or in contact with another vehicle component

Loose U-bolt |
| 1. Tires
 |
| Defect(s)* Damaged tread or sidewall of tire
* Tire leaking (if leak can be felt or heard, tire is to be treated as flat)
 | Major Defect(s)* Flat tire
* Tread depth is less than wear limit
* Tire is in contact with another tire or any vehicle component other than mud-flap
 |
| 1. Wheels, Hubs and Fasteners
 |
| Defect(s)* Hub oil below minimum level. (When Fitted with sight glass)
 | Major Defect(s)* Wheel has loose, missing or ineffective fastener
* Damaged, cracked or broken wheel, rim or attaching part
* Evidence of imminent wheel, hub or bearing failure
* Leaking wheel seal
 |
| 1. Windshield Wiper/Washer
 |
| Defect(s)* Control or System malfunction
* Wiper blade damaged, missing or fails to adequately clear driver’s field of vision
 | Major Defect(s)When necessary for prevailing weather conditions* Wiper or washer fails to adequately clear driver’s field of vision in area swept by driver’s side wiper
 |