|  |  |
| --- | --- |
| 1. Air Brake System | |
| Defect(s)   * Audible air leak * Slow air pressure build up rate | Major Defect(s)   * Pushrod stroke of any brake exceeds the adjustment limit * Air loss rate exceeds prescribed limit * Inoperative towing vehicle(tractor) protection system * Low air warning system fails, or system is activated * Inoperative service, parking, or emergency brake |
| 1. Cab | |
| Defect(s)   * Occupant compartment door fails to open | Major Defect(s)   * Any cab or sleeper door fails to close securely |
| 1. Cargo Securement | |
| Defect(s)  Insecure or improper load covering (e.g. wrong type or flapping in the wind. | Major Defect(s)   * Insecure cargo * Absence, failure, malfunction or deterioration of required cargo securement device or load covering |
| 1. Coupling Devices | |
| Defect(s)   * Coupler or mounting has loose or missing fastener | Major Defect(s)   * Coupler is insecure, or movement exceeds prescribed limit * Coupling or locking mechanism is damaged or fails to lock * Defective, incorrect or missing safety chain/cable |
| 1. Dangerous Goods | |
| Defects(s) | Major Defect(s)   * Dangerous Goods requirements not met |
| 1. Driver Controls | |
| Defect(s)   * Accelerator pedal, clutch, gauges, audible and visual indicators or instruments fail to function properly | Major Defect(s) |
| 1. Driver Seat | |
| Defect(s)   * Seat is damaged or fails to remain in set position | Major Defect(s)   * Seatbelt or tether belt is insecure, missing or malfunctions |
| 1. Electric Brake System | |
| Defect(s)   * Loose or insecure wiring or electrical connection | Major Defect(s)   * Inoperative breakaway device * Inoperative brake |
| 1. Emergency Equipment & Safety Devices | |
| Defect(s)   * Emergency equipment is missing, damaged or defective | Major Defect(s) |
| 1. Exhaust System | |
| Defect(s)   * Exhaust leak | Major Defect(s)   * Leak that causes exhaust gas to enter the occupant compartment |
| 1. Frame and Cargo Body | |
| Defect(s)   * Damaged frame or cargo body | Major Defect(s)   * Visibly shifted, cracked, collapsing or sagging frame member(s). |
| 1. Fuel System | |
| Defect(s)   * Missing fuel tank cap | Major Defect(s)   * Insecure fuel tank * Dripping fuel leak |
| 1. General | |
|  | Major Defect(s)   * Serious damage or deterioration that is noticeable and may affect the vehicle’s safe operation |
| 1. Glass and Mirrors | |
| Defect(s)   * Required mirror or window glass fails to provide the required view to the driver as a result of being cracked, broken, damaged, missing or maladjusted * Required mirror or glass has broken or damaged attachments onto vehicle body | Major Defect(s) |
| 1. Heater/Defroster | |
| Defect(s)   * Control or system failure | Major Defect(s)   * Defroster fails to provide unobstructed view through the windshield |
| 1. Horn | |
| Defect(s)   * Vehicle has no operative horn | Major Defect(s) |
| 1. Hydraulic Brake System | |
| Defect(s)   * Brake fluid level is below indicated minimum level | Major Defect(s)   * Parking brake is inoperative * Brake boost or power assist is inoperative * Brake fluid leak * Brake pedal fade or insufficient brake pedal reserve * Activated (other than ABS) warning device * Brake fluid reservoir is less than ¼ full |
| 1. Lamps and Reflectors | |
| Defect(s)   * Required lamp does not function as intended * Required reflector is missing or partially missing | Major Defect(s)  When Lamps are required:   * Failure of both low-beam headlamps * Failure of both rearmost tail lamps   At all times:   * Failure of a rearmost turn-indicator lamp * Failure of both rearmost brake lamps |
| 1. Steering | |
| Defect(s)   * Steering wheel lash (free-play) is greater than normal | Major Defect(s)   * Steering wheel is insecure, or does not respond normally * Steering wheel lash (free-play) exceeds required limit |
| 1. Suspension System | |
| Minor Defect(s)   * Air leak in air suspension system * Broken spring leaf * Suspension fastener is loose, missing or broken | Major Defect(s)   * Damaged (patched, cut, bruised, cracked to braid, mounted insecurely) or deflated air bag * Cracked or broken main spring leaf or more than one broken spring leaf * Part of spring leaf or suspension is missing, shifted out of place or in contact with another vehicle component   Loose U-bolt |
| 1. Tires | |
| Defect(s)   * Damaged tread or sidewall of tire * Tire leaking (if leak can be felt or heard, tire is to be treated as flat) | Major Defect(s)   * Flat tire * Tread depth is less than wear limit * Tire is in contact with another tire or any vehicle component other than mud-flap |
| 1. Wheels, Hubs and Fasteners | |
| Defect(s)   * Hub oil below minimum level. (When Fitted with sight glass) | Major Defect(s)   * Wheel has loose, missing or ineffective fastener * Damaged, cracked or broken wheel, rim or attaching part * Evidence of imminent wheel, hub or bearing failure * Leaking wheel seal |
| 1. Windshield Wiper/Washer | |
| Defect(s)   * Control or System malfunction * Wiper blade damaged, missing or fails to adequately clear driver’s field of vision | Major Defect(s)  When necessary for prevailing weather conditions   * Wiper or washer fails to adequately clear driver’s field of vision in area swept by driver’s side wiper |