← BACK TO DASHBOARD

# ⚙️ FIRMWARE UPDATE

📌 Instructions:

1. Build your firmware in Arduino IDE or PlatformIO

2. Export the compiled binary (.bin file)

3. Select the .bin file below and click UPDATE

4. Wait for upload to complete (ESP32 will reboot automatically)

⚠️ Do not power off during update!

📁 Select Firmware File (.bin):
0%
⚠️ Warning: This will replace the current firmware. The ESP32 will reboot and may take 30-60 seconds to come back online. Do not close this page until update completes.

💡 Need to update web files?

Use the HMI / Web Files Update page for updating HTML, CSS, and JavaScript files without changing firmware.

→ Go to Web Files Update