**Recommended maximum fill rates**

[Note: these rates are expressed as filling rates of Liters per hour – only the top overflow pipe changes in diameter, regardless of the size of the bottom flange, or side flange if filled via this]

|  |  |
| --- | --- |
| **Diameter of TOP OVERFLOW pipe** | **Maximum fill rate (per HOUR)** |
| 20mm | 1600L/hr |
| 40mm | 6000L/hr |
| 50mm | 10000L/hr |
| 80mm | 22000L/hr |
| 110mm | 40000L/hr |
| 125mm | 62000L/hr |
| 140mm | 77000L/hr |
| 160mm | 100000L/hr |
| 200mm | 158000L/hr |