 **BATTING SEAM TAPE INSTRUCTIONS**

**As with all fusible, please test the Batting Seam Tape and you’re batting before starting your project.**

**Iron Setting: Use steam iron with metal sole plate. Hand-held steamers will not permanently bond Battings Seam Tape to batting. All battings are different and some use heat-set binders to hold them together. In general, the wool setting will work best with most cotton, wool, bamboo, and 80/20 cotton ply blends. Use the silk or synthetic setting with 100% polyester battings, increasing the heat as necessary to ensure a successful bond.**

1. **Join pieces of batting or fabric, lining up the edges closely together.**
2. **Apply Batting Seam Tape over the seam with the fusible (rough side) down.**
3. **Press firmly for 10 seconds then lift the iron (do not slide) and press the next section for 10 seconds overlapping the previously fused area slightly.**

**Repeat, lifting and slightly overlapping iron until all of the Batting Seam Tape is fused. Let batting and tape cool, then check the bond.**

****