 **CRAF-TEX**

**GENERAL INSTRUCTIONS FOR CRAF-TEX FUSIBLE AND CRAF-TEX LITE**

**Cut CRAF-TEX or CRAF-TEX Lite as necessary for your project.**

**1. Place interfacing on the wrong side of the fabric to be fused.**

**2. Fuse-Cover with a damp press cloth. Set iron on low/perm press setting. Press firmly for up to 10 seconds. \***

**Repeat, lifting and slightly overlapping iron until all interfacing is fused.**

**Let fabric cool, then check bond. Use steam iron with metal sole plate. Hand-held steamers will not permanently bond interfacing to fabric.**

**\*Use your damp press cloth as a temperature and timing guide. After 10 seconds, press cloth should be dry. If not, raise iron temperature or hold iron in place a few seconds longer. If the interfacing does not adhere, raise iron temperature slightly. Steam and press to restore or set shape**

**Can be Machine washed and dried.**

**Works with any fabric**

**Can be sewn or fused into any project**

 ****