ENGINE START
Exterior Inspection/ Cockpit set up	COMPLETE
Parking Brake	ON
Doors	CLOSED/ LIGHT OFF
PAX Brief	COMPLETE
Annunciator Panel	Appropriate
Anti-Collision Light	RED
Boost Pump	ON
Engine	2, 3, 1 Start
Engine Parameters	CHECKED

AFTER START/ BEFORE TAXI
DC Power Selector	NORMAL
External Power	DISCONNECTED
Circuit Breakers	IN
Bus Tie	FLIGHT NORMAL /LIGHTS OUT
Electrical Volts/Amps	CHECKED
Engine Controls	CHECKED
Fuel Panel	6 ON/ 4 CLOSED
Bleed Air	TESTED/ CHECKED
Compass	COMPARE
Windshield Heats	NORMAL/ ON
*Anti-Ice 	TESTED / SET FOR TO
Cockpit Lighting	AS REQUIRED
EMER Horizon	ON
Altimeters	SET
GPWS	TESTED
Anti Skid	TESTED
Hydraulics	2 PRESSURES 2 QUANTITES
Hydraulic Standby Pump	ON
*No 1 Stall	Tested
Auto Pilot	CHECKED/DISINGAGED
Yaw damper	AS REQUIRED
Transponder/TCAS	TA/ Tested
Slats/Flaps	CYCLED/SET FOR T.O.
Flight Director & Instruments	BRIEFED
T.O. Briefing	BRIEFED
Masks & Oxy	CHECKED
DV Window	CLOSED





TAXI
Parking Brake	OFF
Taxi Light	ON
Brakes 1&2	CHECKED/ #1& ON
Thrust Reverser	CHECKED/ STOWED
*Engine Computers	CHECKED/ ON
Flight Controls	CHECKED
Xpndr, TCAS	TA
Radar	AS REQUIRED

BEFORE TAKEOFF
Parking Brake	IN/ LIGHT OUT
APU& Bleed air	CONFIRM OFF
Start Selectors	AIR START
Exterior lights	SET
FATSP	CHECK
 
LINE UP CLEARED FOR TAKE OFF
Pitot Heats	ON
Landing Light	ON
Warning Panel / Flags	CLEAR
Engine Instruments	RNWY Heading ALT

CLIMB
LDG Gear/ Taxi Light/ YD	UP OFF ON
Slats & Flaps	CLEAN
Start Selectors	GROUND START
Anti-ice	AS REQUIRED
Cabin Pressure	CHECK
Cabin Temp	CHECKED
Hydraulics	CHECK
Climb Power	CHECK






* First Flight of The Day



N980DM  FALCON 50
10K CHECKS
Lights	SET
No Smoking Seat Belts	AS REQUIRED
Stby Hyd Pmp	AUTO

18K CLIMB/ CRUISE/ STATION
Masks/ Oxy	CHECK
Altimeters	29.92
Circuit Breakers	CHECK
Gen/ Volts/Amps	CHECK
Fuel Panel	CHECK
Anti-ice systems	AS REQUIRED
Ext Lts. / S. Belts/ No Smoking 	AS REQUIRED
Engine Parameters	CHECK
Cabin Press / Temp	CHECK
Hydraulics	CHECK

DESCENT
Cabin Door Curtain	AS Required
Cabin Controller	SET
Anti-icing.	AS REQUIRED
Land Data/ Bugs	COMPLETE / SET
ATIS	NOTED
Risk Assessment	BRIEF
Fuel Panel XFR Intercom/X-feed    	CLOSED

	25
	26
	27
	28
	29
	30
	31
	32
	33
	34
	35

	106
	108
	110
	112
	114
	116
	118
	120
	121
	123
	125



18K DESCENT/ APPROACH
Altimeters (at transition)	SET/CROSS CHECK
Circuit Breakers	CHECK
Gen/ Volts/Amps	CHECK
Anti-ice	AS REQUIRED
Ext lights/ Belts/ Smoke Lights AS REQUIRED 
LDG Light	AS DESIRED
Engine Parameters	CHECK
Cabin Press / Temp	CHECK
Hydraulics/ STBY Pump	CHECK/ON
FMS/Avionics	CHECK/ SET
Radio Altimeter	SET
Approach Brief	COMPLETE
Crew/ PAX Brief	COMPLETE
Start Selectors	AIR START/IGN ON
BEFORE LANDING
Landing Gear/ Anti-skid	DOWN / CHECK
Slats–Flaps	LDG POSITION
Airbrakes	IN/LIGHTS OUT
Yaw Damper	AS REQUIRED
Warning Panel	CHECK
Hydraulics	CHECK
Auto Pilot	OFF
Taxi Light	ON CLEARED TO LAND

AFTER LANDING
Pitot/ Windshield Heat	ALL OFF
Anti-ice	WING OFF/ ENG AS REQ
Ignition	GRD START
Bus Tie	TIED
APU (as applicable)	MASTER/ GEN/ START
Landing Lights, Strobes	OFF
Air Brakes	0
Slats/ Flaps 	CLEAN
Thrust Reversers	STOWED
Trim	SET FOR TAKEOFF
Radar/ Transponder	OFF/ AS REQ
APU/ Bleed Air	AS REQ

PARKING
Taxi Light	OFF
Parking Brake	SET
STBY Pump	OFF
Engines	CUT OFF
Fuel Panel	SET
Anti Collision Light	OFF
Seat Belts/ No Smoking Light	AS REQ
Transponder	AS REQ
Flight Time/ Fuel Burn	RECORD





* First Flight of The Day



SHUTDOWN
APU	SHUTDOWN
Boost Pumps	OFF
NAV Lights	OFF
Seatbelt/ Emer Lights/ cabin	OFF
Cabin Lights	OFF
FMS/ Avionics Masters	OFF
Emerg Battery	OFF
Interior lights	SET
Bus Tie	FLIGHT NORMAL
Pilot window	CLOSED
APU Master	OFF
BAT 1 and BAT 2	OFF
Bus C & D	OFF
Chocks/ Parking Brake	IN / RELEASE

QUICK TURN
FMS Flight time / Fuel	RECORD / ZERO
Clocks	ZERO
Fuel Quantity / Counters 	CHECKED / ZERO
Cabin Press 	SET
Clearance and Code 	COPY AND SET
FMS	LOAD/SET
TOLD/ Vspeeds	COMPLETE/ SET
Engines	START
Bus Tie	FLIGHT NORM
Generator Amps/Volts	CHECK
Windshield Heats	ON
Anti-ice	AS REQ
Warning Panel	CHECK
Slats–Flaps	SET FOR TAKEOFF










Passenger briefing Smoking Seatbelts.
Emergency exits and entry door 
Emergency exits diagram 
Survival equipment
Flotation equipment &Ditching
Oxygen equipment
Briefing cards
FUELING
LO level 13,195 lbs High 15,514 lbs

PROFILE
Climb 260/.72 849
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N980DM Falcon 50 Normal Checklist
Oct 11 2026 Orig
image1.png
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0 5 10 15 20 25 30 35 40 | 45
45 | 9%.1
40 | 96.3
35 | 965 | 96.6
30 | 9.8 | 968 | 97.0
25 | 970 | 970 | 97.2
20 | 972 | 973 | 974 | 975
15 | 97.0 | 975 | 976 | 97.8
10 | 9.1 | 977 | 97.9 | 980 | 98.1
5 953 | 980 | 98.1 98.2 98.4 98.0
0 | 944 | 982 | 983 | 985 | 986 | 983 | 98.0
-5 935 | 974 | 986 | 98.7 98.8 98.5 98.2
-10 | 926 | 965 | 988 | 989 | 99.0 | 987 | 984 | 980
-15 | 91.8 | 957 | 99.0 | 99.1 99.3 99.0 98.6 982 | 982 | 982
20 | 909 | 948 | 991 | 994 | 995 | 992 | 989 | 984 | 984 | 984
-25 99.7 99.4 00.1 98.6 | 986 | 98.6
-30 1000 | 996 | 993 | 989 | 988 | 9838
-35 99.9 99.6 99.1 | 99.0 | 99.0
-40 998 | 993 | 993 | 99.3
-45 1000 | 996 | 995 | 99.5
50 998 | 997 | 99.7

For Climb 300 Kts/.80 MI : Add 0.2% N1
Max ITT: 885°C for 30 min. Max recommended ITT: 849°C.
Area is N1 Value For ISA Conditions





