**MIDWEST CLASSIC STOCKCAR ASSOCIATION**

**2023 Rules**

1. **HAVE FUN!!! This is most important!**
2. Cars and drivers must meet ALL safety rules.
3. All cars will display Association sticker.
4. ONE DRIVER PER NIGHT. ***A non-member may drive a car for free once, 2nd  time pays associate membership fee of $10, 3rd time becomes member and pays remaining $15*** A Driver holding another Sanctioning body license (I.E. IMCA, NASCAR) can only race a total of 2 times with our group unless with prior approval. **ALL SUBS MUST BE APPROVED BEFORE RACING AND WILL READ AND SIGN C.O.C.**
5. Drivers must be at least 16 years old, (under18 with parent’s consent)—ALL drivers must have a valid driver’s license and vision restrictions must be followed to race!
6. No alcohol/drugs/medications that alter your reflexes or reaction time, (including over the counter medications).
7. Drive with the guy in front of you. (Penalties will be assessed on an individual basis.)
8. Cars need to run tight in a group, back off if there is not a car beside you or challenging you from behind. If someone is consistently running way ahead of the pack, they will be subject to a restrictor plate or THROTTLE STOP. **MIRRORS are allowed so you can see the other cars.**
9. ***Once you have won a feature race, you will start in the back and will be disqualified from winning at the next 2 events you attend* (Car and Driver) *All non-winners will be on draw/redraw system. Previous winners will start behind them***
10. **Race receivers REQUIRED.**
11. We know that there may be disagreements from time to time, but let’s try to get along and remember RULE #1 is why we’re here!!!!
12. Membership fee for the year is $25. Must be paid before racing, unless prior arrangements have been made.
13. ***ALL Drivers must read and sign Rules of Conduct and Competition before being allowed to race!***

# SAFETY EQUIPMENT…Let’s keep everyone SAFE!!

1. SFI approved **NECK BRACE AND FIRE SUIT is mandatory**. RACING GLOVES ARE MANDATORY, RACING SHOES ARE RECOMMENDED
2. Fire extinguisher fastened down (within driver’s reach) Recommended
3. Good (3) inch – five (5) point harness, *Must be no older than 4 years old!*
4. DOT approved full-face helmet with shield.
5. SFI approved fuel cell is mandatory, with tip-over valve, no PCV type valves allowed. Fuel cell with can recommended.
6. Fully enclosed firewall between fuel cell and driver.
7. Window net or arm restraints.
8. Top must be enclosed over the driver, (no convertibles, and no sun roofs).
9. Doors must be fastened shut.
10. Fan shroud mandatory.
11. Battery must be fastened down and in a plastic boat box if it is in the driver’s compartment. If it is in the trunk, it must be securely fastened down behind the firewall.
12. Six point roll cage of minimum 1 5/8 tubing on main bars, (no exhaust tubing cages), mandatory door bars (minimum of 3). If the car had an existing roll cage, check it carefully, they often rust from within. Driver’s door plate of minimum 18 gauge steel recommended.
13. Electric fuel pumps are only allowed on flathead engines, it must have a mercury or inertia switch, running light, and well-marked kill switch.
14. **MANDATORY – IGNITION KILL SWITCH WITHIN DRIVERS REACH WHEN YOU ARE BELTED IN. Clearly marked ON/OFF. A MASTER POWER SWITCH is recommended for all cars.**
15. ***Aluminum Racing Seat Mandatory!***
16. Numbers and accompanying letters (i.e. 4x, 2m, etc.) Must be at least 2” wide and at least 18” tall and on both sides of the car in contrasting colors. (letter can be smaller)
17. Solid motor mounts not required, but highly recommended. ***NO Excessive engine setback! Front sparkplug can be no further back then even with the upper balljoints!***
18. Solid front firewall and full floor from firewall to rear of cage is required, (non factory floor is ok). 18 gauge sheet metal minimum, NO aluminum floor under driver’s seat. Interior may be dog housed in, ***floor is not necessary under the doghouse***
19. If fuel line runs through driver’s compartment, must be enclosed in conduit. Steel or braided racing line recommended.
20. Cars will be inspected before competing and may be inspected at any time.

**FRAME and BODY**

1. OEM frames only!! No full tubular frames. Frame does not have to match body. No wheelbases shorter than 105”. ***Rear tubular frame allowed if suspension mounts in stock position.* Must have stock front stub! Front upper control arm mounts may be altered and moved.**
2. **Stock intent suspension, front and rear.** Tubular Upper Control Arms allowed. Weight jacks are allowed. *Pan hard bars allowed, as long as mounted in a stock configuration. NO Excessive angles. May be curved for clearance, but absolutely NON-ADJUSTABLE!!* No coil-over or torsion suspension, NO half leafs, No fifth arm or pull bars on rear end, NO traction bars.
3. Shocks – one per wheel, except for RF, which may be double shocked.
4. Good working four wheel brakes. Random testing may be performed. Brake adjuster is ok from front to back. NO on/off switch.
5. Steering – must have a steering box, can use power steering or rack and pinion.
6. TIRES – MAX 9.5” mounted on 8” or smaller rim. You may use racing or standard tires. No snow or mud tires. No unilug wheels. Beadlock on RR only.
7. Frame – if you replace it, it must have OEM frame rails (truck frame o.k.) and OEM width. Keep the frame in proportion to the body
8. Body: The body must be an American made***, 1949-1977 GM 49-79 Ford/Mopar***.  *Fiberglass STOCK appearing roofs allowed. Must match body (E.G. 55 Chevy Kit Body) Aluminum replacement panels allowed as long STOCK appearing.* **Bodies subject to approval before racing**! ***No Pickups***. The body must be of original width, but may be shortened (to an extent) to match frame wheelbase. Doors, hood and trunk lid must fasten securely. NO wings. **Max 6” spoiler**.
9. The car should be kept looking good, painted, clean and presentable in appearance. Keep the cars looking like old race cars…**motor close to stock position, front sparkplug to stay even with or ahead of upper balljoints,** radiators in the front.
10. Bumpers – must have front and rear bumpers and must be securely fastened. Do not have to be stock, may be tubular**. *Nosepiece allowed with prior approval! prefer not to have them.***
11. ***3150lbs minimum weight with Driver!*** If weight blocks are used, they must be secured with 1/2" bolts; weights must be painted white and have the car number on them
12. Rub rails are allowed, but better never be used!!!
13. All Cars Should display what they are either on visor or grandstand side of car. Ex: 1964 Pontiac Le Mans, 1953 Chevy etc.

**DRIVE-TRAIN**

1. V-8 American made block, NO cubic inch rule. Block and heads must be cast iron.
2. ***Holley 4412 Carburetor Mandatory***. **MUST BE ABLE TO PASS GUAGE TEST!! Must have choke horn, Aftermarket metering block allowed. Race Fuel, Alcohol, E85, or Pump Gas Only.**  **OEM aluminum, cast iron, or aftermarket aluminum intake that measure no more than 6 ½ inches from bottom of back of intake to carburetor. This includes any adaptor/ spacer!** **Spacer/Adaptor not to exceed 1 inch!**
3. ***MAXIMUM of Flat Top Pistons only!*** Any exhaust, any ignition. ROLLER ROCKERS or ROLLER TIP ROCKERS are allowed, but NO Roller cams or lifters! NO fuel injection OR turbo chargers.
4. Inline 6 – American made stock automotive parts only. Crank MUST match OEM stroke. One unmodified Holley 4412, with no more than a one inch spacer or one inch, adapter under the carburetor. Cast iron head. Any exhaust, any ignition. No aftermarket cranks. No stroker motors, NO ROLLER CAMS or ROLLER LIFTERS allowed! NO fuel injection OR turbo chargers.
5. Flathead V-8 – Flatheads can do anything they want, multi carbureted. Basically, whatever you can afford!!
6. **Transmissions must be OEM** – any automatic. Any 3, 4 or 5 speed with clutch in blow-proof bell housing! Clutch pedal or hand clutch allowed – with working reverse. No in and out boxes. Torque Convertors optional.
7. Rear ends – any rear end, 3/4 ton truck, locked, full floating, or quick change with steel tubes are allowed. NO independent rear suspension allowed.
8. Driveshaft – must be painted white and must have a driveshaft loop, not over 6” from front u-joint. Second loop constructed of cable or chain in the rear, recommended
9. Must have a working starter.

**DO NOT READ BETWEEN THE LINES. IF IT DOESN’T SAY YOU CAN DO IT….YOU CAN’T!!!**

**Contact Eric Cerny @ 402-615-2840 or Mike Ganskow @ 402-910-0164**

**Or email** [**MCSA00@live.com**](mailto:MCSA00@live.com) **with any questions.**