TIPTON PLANT LAYOUTCircular Drive
Oil 
Shop Area
L
P

Tank
Power
Box
506
505
504
503
502
Fuel
Tanks
Driveway
Electrical 
Building

518

PKG Chemicals
Electrical 
Panel 

 Trough
Junge
Mixer
Junge
Mixer
Mini Bulk Chemicals
519
1483
Driveway

AC

    Office
Water
Bulk Chemical Dike
Fertilizer Dike
508
515
501
514
507
Loading Pad
Overhead Tanks
511
510
509
513
512



Hwy 130


Air
Compressors
Oil
Metholine
Anti-Freeze
Mixer

TIPTON PRODUCT LOCATION	

Tank #		Product		Circumference		   Gallons/inch		Weight

501			3-10-30		25,000 Gal (12’x30’0		70.49				12.64
502			10-32-0/2		25,000 Gal (12’x30’)		70.49				11.75
503			28% or 32%		30,000 Gal (12’x35)		70.49		      10.64 or 11.04
504			28% or 32%		30,000 Gal (12’x35)		70.06		      10.64 or 11.04
505			28% or 32%		30,000 Gal (12’x35)		70.49		      10.64 or 11.04
506		12-0-0-26 or 11.08-0-0-24	25,000 Gal (12’x30’)		70.49		       11.04 or 10.77
507			Zinc 15%		2,600 Gal Poly Tank						10.78
508						3,000 Gal Poly Tank						
509	143”		Instinct NXTGEN	2,400 Gal		(16.66Gal/inch) (33 Gal in cone)		9.639
510	119”		Keystone NXT	2,000 Gal		(16.66Gal/inch) (33 Gal in cone)		9.268
		Or	Harness Xtra 5.6L										9.274
511	143”		Atrazine 4L		2,400	Gal		(16.66Gal/inch) (33 Gal in cone)		9.2
512	144”		Roundup Powermax 3	2,575 Gal		(17.62 Gal/inch) (37.33 Gal in cone)	           11.5167
513	48.5”		Resicore REV	1,000 Gal		(H/48.5) x 1,000				9.1215
514			Poly-Plex		1,500 Gal								11.04
515						1,500 Gal								
518			Taurus Sulfur	1,500 Gal								10.4
519			Clay			2,600 Gal								9.63






Note: inches X gallons per inch X weight = lbs / 2000 = tons				Rev. 01/16/2026
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