Tanker 3

#912 1992 GMC E-One Tanker

Updated 4/1/2014 WTL

Compartment Under Pump Panel

1- 50’ Supply Line

1- Male Quick Coupling

1- Female Quick Coupling

1- Double Male

1- Double Female

Rear Compartment

1- 2 ½ Barrel

2- Spanner

1- Pickhead Axe

1- Flathead Axe

1- Female Quick Connect

1- Hydrant Wrench

Hose Bed

200 ft 2 ½

100 ft 1 ¾

1- 1 ¾ Fog Nozzle

Passenger Side

1- Dump Tank

Driver Front Compartment

2- Handlights

1- 20 lb ABC fire extinguisher

1- 1 ½ Fog Nozzle

1- Rubber Hammer

Booster Reel Wrenches

2- 5” Spanner Wrench

2- 2 ½ Spanner Wrench

1- Hydrant Wrench

Driver Side Middle Compartment

2- SCBA Airpacks

Driver Side

1- Straight Dump Tube

1- 90 Deg. Dump Tube

2- 2 ½ Hard Suction

2- Female Quick Connect

2- Male Quick Connect

1- 12ft Pike Pole

1- 3ft Pry Bar

Driver Side Rear

6- Traffic Cones

10- 5gal Foam

1- 5” Quick Fill

Curb Side/ Passenger Side

Pump Panel 2 ½ Quick Connect Female

1- 2 ½ Double Male

1- 2 ½ Double Female

1- Quick Dump Tank

Under Pump Box

1- 50’ Rubber Filler Line w/ Quick Connect Male/Female

2nd Compartment Lower

2- 5gal Class A Foam

3rd Compartment Lower

2- 5gal Class A Foam

1- 50 2/1/2 Cloth Filler Line w/ Male Quick Connect

1- 4” PVC Quick Dump Connecter W/ Accessories

1- 2 ½ Gate Valve Screw Type

Step Right Conner

1- Pick head Axe

Top Over Pump Panel

6- 5 gal Class A Foam

Cab

2- Traffic Vest

1-UHF Mobile radio

1-800mhz Mobile radio