

**HOW TO RECEIVE A MESSAGE IN THE PEER-TO-PEER MODE**

1. Open the Winlink Express application
2. Select *Packet P2P* in the *Open Session* box
3. You are now ready to receive Peer-to-Peer messages





**HOW TO SEND A MESSAGE IN THE PEER-TO-PEER MODE**

1. Open the Winlink Express application.
2. Select *Packet P2P* in the *Open Session* box
3. Click *Message / New Message*



1. The *Enter a new message* window should open as seen below
2. Type the callsign of the receiving station in the *To* field
3. Type the *Subject*
4. Type the message to be sent
5. Select *Peer-to-Peer* in the *Send as* box
6. Click *Post to Outbox*
7. Click *Open Session* (Packet P2P)



1. The *Packet Peer-to-Peer Session* screen should open, and the TNC will be initialized.
2. When you see *Ready*, click ***Start*** and the message will be sent to the receiving station.
3. If the receiving station has any email in their Outbox for your station, you will receive that email.

