Original 2 Wires

**B1 I B**

 **L**

 From

 Original Key Switch

 **I & B**

 Special 3 Position Key Switch

 0 0

 Brake Light Switch

 **+**

 12 Volt

 Power

 +

 Fuse

1. Mount brake light switch and bracket above brake pedal under the front of the cart.
2. Replace Cart key switch with new 3 position switch.
3. Connect 12 Volt power supply to fuse holder and terminal B1 on key switch with supplied green wire.
4. Connect supplied Brown wire from Key switch L to one terminal on brake light switch.
5. Connect supplied brown wire from other terminal to tail lights 3rd wire each side.
6. Connect carts original key switch 2 wires to terminals I & B.
7. When key is turned to the right 1 position only the cart will operate, turn key to position 2 and the brake light switch will have power. When the cart is parked with the key switch off will prevent the brake lights staying on.

# \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# EDGEWATER CUSTOM GOLF CARTS

**4890 Edgewater Dr Orlando Florida 32804 Parts List**

 **407 295-3279** Key Switch Green Wire

 **edgewatercustom@hotmail.com**  Brake Light Switch Brown Wire

 Bracket Wire Ties

 Fuse & Holder Terminals

**Key Switch Brake light Kit Parts**

Red Hawk Switch # Key-51

B/L Switch

Plastic Bracket

Fuse Holder

Fuse

12’- Green Wire

18’- Brown Wire

6- Female Spade Terminals

2- #6 Ring Terminals

1-5/16 Ring Terminal

4- Blue Barrel Terminals

Diagram