South STREET North

 L-3 L-2

 Ckt #3

 LC Motor #1

 Nothing done to

 these existing JB’s !

 Ckt #7, Motor #2 Photo Cell ( L-1 & L-2 )

 Sprinkler #2 L-3 Sprinkler #1

 b)- J.B. L-1 a)- J.B.

 PVC Main J.B. ( parking Lights ) ( Future Use ) ( Parking Lights )

 Ckt # 5 Ckt # 1

Load Center fed from House Meter Main Disconnect… “ Two Pole 60 Amps “ .

All electrical wiring was done with #12 AWG ( Stranded ) .

All electrical conduit : ½ “ PVC electrical conduit .

All Breakers : 20 Amp / Single Pole / 120 Volts … Interrupting rating .