South STREET North

L-3 L-2

Ckt #3

LC Motor #1

Nothing done to

these existing JB’s !

Ckt #7, Motor #2 Photo Cell ( L-1 & L-2 )

Sprinkler #2 L-3 Sprinkler #1

b)- J.B. L-1 a)- J.B.

PVC Main J.B. ( parking Lights ) ( Future Use ) ( Parking Lights )

Ckt # 5 Ckt # 1

Load Center fed from House Meter Main Disconnect… “ Two Pole 60 Amps “ .

All electrical wiring was done with #12 AWG ( Stranded ) .

All electrical conduit : ½ “ PVC electrical conduit .

All Breakers : 20 Amp / Single Pole / 120 Volts … Interrupting rating .