EFFECTIVE GROUNDING FOR LT. POLES AS PER NEC ARTICLE 250

Lt. Pole

Ground Terminal

Ground / surface level ( Electrically bonded to branch circuit grounding )

#6 AWG Grounding Conductor

Ground Clamp ( Oversized … more than requirements of Table 250.122 )

Ground Electrode Rod

5/8” x 8’ ( ft )