¾ “ Electrical PVC . One set of 3 #12 THHN Conductors . 18” Depth .

 South

Trenching

Distance =

200’ ( Ft ) ,

from inside of

building ( Load /

Center ) to

Pole #2 .

 Pole #1 Pole #2

 North