Lexus GS300 [2002] MAF Re-Wiring Configuration To Accept Aristo 2JZ-GTE Stock MAF Sensor

-TERMINAL 1: B+ (BLACK/RED STRIPE) -> TERMINAL 4

-TERMINAL 2: E2G (GRAY) -> TERMINAL 3

-TERMINAL 3: VG (RED/LIGHT BLUE STRIPE) -> TERMINAL 5

-TERMINAL 4: THA (WHITE/RED STRIPE) -> TERMINAL 1

-TERMINAL 5: E2 (BROWN) -> TERMINAL 2

**M 1**

Black

1 2 3 4 5

MAF CONNECTOR TERMINAL SCHEMATIC