TOP SLIDE BRACKET SHIM INSTALLATION

When placing and mounting slide bracket, if bracket will sit completely on the metal deck edge, the included 2” x 2” shims are not needed.

If it is necessary to move the slide bracket back and have sit on floor instead of metal deck edge then the shims are needed. Sometime the deck edge is very narrow and the slide bracket having 2” square feet, will not sit completely and flat on deck edge.

When the slide bracket is placed behind the deck edge on the boat floor, the shims will raise up the slide bracket to compensate for the 1/8” height difference when floor mounted. This also allows the tongue of the mount not to bind.