

|  |  |  |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | **Programming a One Touch Key** |  |  |  |  | | --- | | **\*First you must be sure the button you wish to program is a "One Touch Button" see programming flexible buttons to ensure  1. Press #9876 to enter User Programming Mode 2. Press the One Touch button to be set 3. Enter the digits or special buttons for the function to be dialed - maximum 32 characters - To program a feature access code see: helpful feature codes on this page 4. Press the One Touch button to save the entry** |   **For additional help please call us at 249-248-0000 (Michigan) or 239-561-0090 (Florida)** |