***THE RYCO COMBIBATCH USES HIGH SPEED COMBANATIONAL COMPUTATION TO:***

|  |  |
| --- | --- |
| • Minimize GiveAway  • Minimize labor  • Maximize profit  • Maximize throughput to shipping  • Reduce your GiveAway 3% or less.  • GiveAway reduction drops direct to your  bottom line  Incorporates high accuracy weigh cells  and high reliability Industrial computer to fill  bags to target weights.  Specialized combinational mathematics  allows selection of items to match target  weight. With 6 average items in a batch,  can produce batches with no underweight  and average overweight less than 1.6%.  **FEATURES:**  • 14 selection hoppers  • 30 to 200 gm pieces  • Up to 15 batches per minute  • Highly accurate batch weights  **RYCO ADVANTAGES:**  • Designed to operate in remote plants  • Completely washdown  • Easily serviced by plant mechanics  **OPTIONS:**  • Weigh hoppers up to 4.5 pounds  • Hoppers for round Salmon batching  • Bagging and sealing attachments |  |