**Project Description from Johnny and Mary Randel**

Overview: Installation of Marvin Signature Clad window units to replace existing windows

Description:

Marvin Signature Units

Stone white exterior

PF white interior (except line 1)

Low E 2 with Argon glass

5/8 SDL with black spacer and perimeter bar

Stone white ½ screens double hungs

White screens casement

White hardware

Thru jamb installation