Date \_\_\_/\_\_\_\_\_/\_\_\_\_\_\_\_ Inspector: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Pull: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ Tractor:\_\_\_\_\_\_\_\_\_\_\_\_\_ Driver: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_

The following **6** safety items are mandatory on all tractors to receive a complete inspection for competition.

The absence of any of the following **6** Safety items will result in **Automatic Disqualification**!

Check the following boxes that apply Satisfactory [x]  Unsatisfactory[x]

-Does the tractor have SFI approved clutch? NO Exceptions! Satisfactory [ ]  Unsatisfactory[ ]

-Does the tractor have a wheelie bar that supports weight of tractor with 5 X 5 pads Satisfactory [ ]  Unsatisfactory[ ]  horizontal to the ground?

-Does the tractor have a roll bar or cage that supports the weight of tractor? Satisfactory [ ]  Unsatisfactory[ ]

-Does the tractor have SFI Approved Blanket, or 3/8-inch steel -- ½ inch Satisfactory [ ]  Unsatisfactory[ ]  Aluminum X 6” wide bolted to frame covering bell housing?

-Does the tractor have fuel dump valve that is 3-way dump before injection pump, Satisfactory [ ]  Unsatisfactory[ ]  and is it able to be pulled from seat while strapped in?

-Does the tractor have air shut off that is reachable from seat well strapped in and Satisfactory [ ]  Unsatisfactory[ ]  one on the rear of tractor with the ability to hook to sled? (Mandatory check & Test)

 **Is the tractor Automatically Disqualified YES** [ ]  **NO**[ ]

-------------------------------------------------------------------------------------------------------------------------------------------------------------- --

 Satisfactory Unsatisfactory

-Is the tractor equipped with seat belt or have 5-point harness if equipped with Cage? [ ]  [ ]

- Is the tractor equipped with a neutral safety start? (Must not be able to start well in gear) [ ]  [ ]

- Does the tractor have neutral safety light on rear, clear in color? (Unlimited tractors only) [ ]  [ ]

- Is tractor equipped with 3.5 lbs. Fire Extinguisher? [ ]  [ ]

- Is tractor equipped with a dead man’s throttle with 2 return springs? [ ]  [ ]

- Are the breaks in working condition? (Pump breaks and be sure they hold) [ ]  [ ]

-Is exhaust vertical with 2- 3/8 cross bolts? [ ]  [ ]

-Is Side shields .060 steel or .120 aluminum? [ ]  [ ]

- Is firewall .060 steel or .120 aluminum? [ ]  [ ]

-Is tractor free of metal cooling fan blades? (No Metal Blades on fans) [ ]  [ ]

-Does tractor have 3/8” cable or larger, 360 degrees between cylinder 1 and 2 w/ 4 clamps [ ]  [ ]

-Is the wheel hubs steel or heavy clamp style hubs? [ ]  [ ]

- Draw bar has Horizontal pin 3” X 3.75”? (Hole Must be ridged) [ ]  [ ]

- Does the tractor have tie bars with rear end tied to frame rails? [ ]  [ ]

- Is the tractor equipped with wide front-end ski bars? Mandatory (Except Factory Front Ends) [ ]  [ ]

- Does the tractor have a shield or can withhold the balancer from exiting? [ ]  [ ]

- Is the tractor equipped with a 3 X 3 turbo or smaller? [ ]  [ ]

--------------------------------------------------------------------------------------------------------------------------------------------------- -------------

 **The above tractor qualifies for competition: YES** [ ]  **NO**[ ]

 Inspector: I hereby certify the above tractor for competition. Sign: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Driver: I hereby agree with the above Inspection. Sign: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_