**Manual Control Box Wiring Instructions**

| Pink | 12v ignition |
| --- | --- |
| Brown | Ground through switch for TCC Lock up |
| Yellow/Black | For D1 Transbrake, ground through switch for activation. (If no D1, this will not be used.) |
| Black/Red | For D3 Transbrake wire to ignition power source. (If no D3, this will not be used.) |
| Light blue/white | For D3 transbrake, wire to chassis ground. (If no D3, this will not be used.) |