**Level A Checks
Preventative Maintenance**

**Daily**

* Monitor daily fire weather risk online

**Monthly**

* Tap bottoms of fire extinguishers and ensure charge
* Survey perimeter to identify maintenance issues

**Spring leaf pollen season**

* Check downspouts for clogs and remove debris in gutters clogging downspouts
* As needed, use leaf blower to remove dead leaf matter from driveway and flower beds

**June and November**

* Mow perimeter
* Remove dead limbs from trees around house
* Vacuum out gutters
* Check vents to ensure mesh is still in place
* Use leaf blower to remove any loose debris
* Rake up leaves and pick up sticks

**Level B Checks
During Periods of Extended High Risk**

**Roof**

* Check vents to ensure mesh is still in place
* Use leaf blower to remove any loose debris

**Hose bibs**

* Check hoses and nozzles at all hose bibs

**Use leaf blower to remove dead leaf matter from driveway and flower beds**

**Level C Checks**

**During Active Wildfire Conditions Near Home**

**Conduct all Level A and B checks (except for mowing) at onset of situation**

**Begin Evacuation Checklist and Load Out procedures**

**Move all flammable items from patio to inside**

* Pool toys
* Seat cushions
* Rugs