G-BOOT FAQ



**1. How much does each boot cost?**

 **A. Each boot costs $21 and included the required**

 **fasteners to secure the boot into a wood nailer.**

**2. How much does each G-BOOT weigh?**

 **A. Each plastic boot is easy to handle and weighs**

 **approximately 2.05 pounds.**

**3. Is the G-BOOT reusable?**

 **A. Yes, you can reuse the G-BOOT. Prior to each**

 **installation, the boot should be inspected for crack,**

 **tears, breaks or other damage.**

**4. G-BOOT cost vs. metal guardrail cost.**

 **A. Two G-Boots and 4 – 2x 4’s, to make an 8-foot**

 **section, with labor costs approximately $55. An 8 –**

 **foot section of metal guardrail, with two bases**

 **without labor, costs approximately $155 plus shipping.**

**5. What substrates can the G-BOOT be installed on?**

 **A. The G-BOOT can be used on new construction or**

 **existing buildings and installed directly onto 22-`18Ga.**

 **metal deck, through a wood nailer and into metal deck**

 **and concrete. The competent person is responsible to ensure**

 **the substrate will support the intended load.**

**COPYRIGHT 2019 | SAFETY KEVIN, LLC IS A VETERAN OWNED BUSINESS | KEVIN@SAFETYKEVIN.COM**