**Spektrum Wireless Trainer**

**HOW TO BIND THE MASTER TRANSMITTER TO SLAVE TRANSMITTER**

* 1ST, Bind master transmitter to the airplane.
* Set master transmitter to the settings for the model you are binding too.
* Check all your settings to the plane.
* On the slave transmitter go to “**model select”, “add new model”, then “model type” *select airplane***.  Turn off the slave transmitter.
* On the master transmitter go into **system setup**, go to **trainer**.   In trainer, select **Wireless Trainer**.  Set it to **Pilot Link Master**, then select bind and press to bind.
* Now turn on the slave transmitter while holding down the bind button I.

The two transmitters should now be bound to each other.