#### 7.2.2.13 IfcOutletTypeEnum

The IfcOutletTypeEnum defines the range of different types of outlet that can be specified.

> HISTORY New type in IFC2x.

> IFC4 CHANGE Telephone and Data outlets added.

Enumerated Item Definitions:

- AUDIOVISUALOUTLET: An outlet used for an audio or visual device.
- COMMUNICATIONSOUTLET: An outlet used for connecting communications equipment.
- POWEROUTLET: An outlet used for connecting electrical devices requiring power.
- DATAOUTLET: An outlet used for connecting data communications equipment.
- TELEPHONEOUTLET: An outlet used for connecting telephone communications equipment.
- USERDEFINED: User-defined type.
- NOTDEFINED: Undefined type.

XSD Specification:

<xs:simpleType name="IfcOutletTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="audiovisualoutlet"/>
<xs:enumeration value="communicationsoutlet"/>
<xs:enumeration value="poweroutlet"/>
<xs:enumeration value="dataoutlet"/>
<xs:enumeration value="telephoneoutlet"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>

EXPRESS Specification:

TYPE IfcOutletTypeEnum = ENUMERATION OF (
| AUDIOVISUALOUTLET, COMMUNICATIONSOUTLET, POWEROUTLET, DATAOUTLET, TELEPHONEOUTLET, USERDEFINED, NOTDEFINED);
END_TYPE;

Link to this page