#### 7.2.2.1 IfcCableCarrierFittingTypeEnum

The IfcCableCarrierFittingTypeEnum defines the range of different types of cable carrier fitting that can be specified.

> HISTORY New type in IFC2x2.

Enumerated Item Definitions:

- BEND: A fitting that changes the route of the cable carrier.
- CROSS: A fitting at which two branches are taken from the main route of the cable carrier simultaneously.
- REDUCER: A fitting that changes the physical size of the main route of the cable carrier.
- TEE: A fitting at which a branch is taken from the main route of the cable carrier.
- USERDEFINED: User-defined type.
- NOTDEFINED: Undefined type.

XSD Specification:

<xs:simpleType name="IfcCableCarrierFittingTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="bend"/>
<xs:enumeration value="cross"/>
<xs:enumeration value="reducer"/>
<xs:enumeration value="tee"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>

EXPRESS Specification:

TYPE IfcCableCarrierFittingTypeEnum = ENUMERATION OF (
| BEND, CROSS, REDUCER, TEE, USERDEFINED, NOTDEFINED);
END_TYPE;

Link to this page