#### 7.2.4.4 Pset_CableCarrierSegmentTypeCableTrunkingSegment

PSET_TYPEDRIVENOVERRIDE / IfcCableCarrierSegment / CABLETRUNKINGSEGMENT

| An enclosed carrier segment with one or more compartments into which cables are placed. HISTORY: IFC4 - NominalLength deleted. To be handled as a quantity measure
| 一つ以上の区画にケーブルを収納する密閉型ケーブルキャリアに関するプロパティセット定義。

buildingSMART Data Dictionary

PSD-XML

- NominalWidth
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | NominalWidth: The nominal width of the segment.
  | 公称幅: 呼び幅寸法。
  | 공칭 폭: 폭 치수

- NominalHeight
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | NominalHeight: The nominal height of the segment.
  | 公称高: 呼び高寸法。
  | 공칭높이: 고 치수

- NumberOfCompartments
  P_SINGLEVALUE / IfcInteger

  | NumberOfCompartments: The number of separate internal compartments within the trunking.
  | 区画数: 管の区別される内部区画の個数。
  | 구획 수: 관 구분되는 내부 파티션 개수

Link to this page