#### 7.2.4.25 Pset_LightFixtureTypeSecurityLighting

PSET_TYPEDRIVENOVERRIDE / IfcLightFixture / SECURITYLIGHTING

| Properties that characterize security lighting.
| 防犯灯の特徴プロパティ。

buildingSMART Data Dictionary

PSD-XML

- SecurityLightingType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_LightFixtureSecurityLightingType: SAFETYLIGHT, WARNINGLIGHT, EMERGENCYEXITLIGHT, BLUEILLUMINATION, OTHER, NOTKNOWN, UNSET

  | SecurityLightingType: The type of security lighting.
  | 防犯灯: 防犯灯のタイプ。
  | 방범등: 방범등 유형

- FixtureHeight
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | FixtureHeight: The height of the fixture, such as the text height of an exit sign.
  | 器具の高さ: 出口標識などの器具の高さ。
  | 기구의 높이: 출구 표지판 등의기구의 높이

- SelfTestFunction
  P_ENUMERATEDVALUE / IfcLabel / PEnum_SelfTestType: CENTRAL, LOCAL, NONE, OTHER, NOTKNOWN, UNSET

  | SelfTestFunction: The type of self test function.
  | 自己診断機能: 自己診断機能のタイプ。
  | 자기 진단 기능: 자기 진단 기능의 유형

- BackupSupplySystem
  P_ENUMERATEDVALUE / IfcLabel / PEnum_BackupSupplySystemType: LOCALBATTERY, CENTRALBATTERY, OTHER, NOTKNOWN, UNSET

  | BackupSupplySystem: The type of backup supply system.
  | 電源バックアップシステム: 電源バックアップシステムのタイプ。
  | 전원백업 시스템: 전원 백업 시스템 유형

- PictogramEscapeDirection
  P_ENUMERATEDVALUE / IfcLabel / PEnum_PictogramEscapeDirectionType: RIGHTARROW, LEFTARROW, DOWNARROW, UPARROW, OTHER, NOTKNOWN, UNSET

  | PictogramEscapeDirection: The direction of escape pictogram.
  | 避難標識の向き: 避難標識の向き。
  | 피난 표지판 방향: 피난 표지판 방향

- Addressablility
  P_ENUMERATEDVALUE / IfcLabel / PEnum_AddressabilityType: IMPLEMENTED, UPGRADEABLETO, NOTIMPLEMENTED, OTHER, NOTKNOWN, UNSET

  | Addressablility: The type of addressability.
  | アドレス指定能力: アドレス指定能力のタイプ。
  | 주소 지정 능력: 주소 지정 능력 타입

Link to this page