#### 6.2.4.1 Pset_DistributionPortTypePipe

PSET_TYPEDRIVENOVERRIDE / IfcDistributionPort / CHEMICAL

| Pipe port occurrence attributes attached to an instance of IfcDistributionPort.
| IfcDistributionPortオブジェクトに設定される配管ポートに関する属性情報。

buildingSMART Data Dictionary

PSD-XML

- ConnectionType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_PipeEndStyleTreatment: BRAZED, COMPRESSION, FLANGED, GROOVED, OUTSIDESLEEVE, SOLDERED, SWEDGE, THREADED, WELDED, OTHER, NONE, UNSET

  | ConnectionType: The end-style treatment of the pipe port: BRAZED: Brazed. COMPRESSION: Compression. FLANGED: Flanged. GROOVED: Grooved. OUTSIDESLEEVE: Outside Sleeve. SOLDERED: Soldered. SWEDGE: Swedge. THREADED: Threaded. WELDED: Welded. OTHER: Another type of end-style has been applied. NONE: No end-style has been applied. USERDEFINED: User-defined port connection type. NOTDEFINED: Undefined port connection type.
  | 接続タイプ: 物理ポート接続： - Coaxial: 同軸コネクタ. - DSub: D-Subコネクタ. - Infrared:赤外線 - RJ: 登録済みジャック. - Radio: 無線 - USB: USB.

- ConnectionSubType
  P_SINGLEVALUE / IfcLabel

  | ConnectionSubType: The physical port connection subtype that further qualifies the ConnectionType.
  | 接続サブタイプ: 物理ポート接続のサブタイプ。接続タイプ以外の情報を設定する場合に使用。下記の値を設定： - DSub: DA15, DB25, DC37, DD50, DE9, DE15 - Radio: IEEE802.11g, IEEE802.11n - RJ: 4P4C, 6P2C, 8P8C - USB: A, B, MiniA, MiniB, MicroA, MicroB

- NominalDiameter
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | NominalDiameter: The nominal diameter of the pipe connection.
  | 呼び径: 配管の呼び径。

- InnerDiameter
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | InnerDiameter: The actual inner diameter of the pipe.
  | 内径: 配管の実内径。

- OuterDiameter
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | OuterDiameter: The actual outer diameter of the pipe.
  | 外径: 配管の実外径。

- Temperature
  P_BOUNDEDVALUE / IfcThermodynamicTemperatureMeasure

  | Temperature: Temperature of the fluid.
  | 温度: 流体の温度。

- VolumetricFlowRate
  P_BOUNDEDVALUE / IfcVolumetricFlowRateMeasure

  | VolumetricFlowRate: The volumetric flow rate of the fluid.
  | 体積流量: 流体の体積流量。

- MassFlowRate
  P_BOUNDEDVALUE / IfcMassFlowRateMeasure

  | MassFlowRate: The mass flow rate of the fluid.
  | 質量流量: 流体の質量流量。

- FlowCondition
  P_BOUNDEDVALUE / IfcPositiveRatioMeasure

  | FlowCondition: Defines the flow condition as a percentage of the cross-sectional area.
  | 流動状態: 断面の充満率で流動状態を定義する。

- Velocity
  P_BOUNDEDVALUE / IfcLinearVelocityMeasure

  | Velocity: The velocity of the fluid.
  | 速度: 流体の速度。

- Pressure
  P_BOUNDEDVALUE / IfcPressureMeasure

  | Pressure: The pressure of the fluid.
  | 圧力: 流体の圧力。

Link to this page