#### 7.3.4.11 Pset_PipeConnectionFlanged

PSET_TYPEDRIVENOVERRIDE / IfcPipeSegment

| This property set is used to define the specifics of a flanged pipe connection used between occurrences of pipe segments and fittings.

buildingSMART Data Dictionary

PSD-XML

- FlangeTable
  P_SINGLEVALUE / IfcLabel

  | FlangeTable: Designation of the standard table to which the flange conforms.
  | フランジ基準: フランジ形状の名称基準

- FlangeStandard
  P_SINGLEVALUE / IfcLabel

  | FlangeStandard: Designation of the standard describing the flange table.
  | フランジ規格: フランジ規格を記述している基準

- BoreSize
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | BoreSize: The nominal bore of the pipe flange.
  | フランジの内径のサイズ: フランジの呼び径

- FlangeDiameter
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | FlangeDiameter: Overall diameter of the flange.
  | フランジの直径: フランジの全直径

- FlangeThickness
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | FlangeThickness: Thickness of the material from which the pipe bend is constructed.
  | フランジの厚さ: パイプをつなぐ材料の厚み

- NumberOfBoltholes
  P_SINGLEVALUE / IfcInteger

  | NumberOfBoltholes: Number of boltholes in the flange.
  | ボルト穴の数: フランジにあるボルト穴の数

- BoltSize
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | BoltSize: Size of the bolts securing the flange.
  | ボルトの大きさ: フランジを締めるボルトの大きさ

- BoltholePitch
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | BoltholePitch: Diameter of the circle along which the boltholes are placed.
  | ボルト穴ピッチ: ボルト穴がある円の直径

Link to this page