#### 7.3.4.30 Pset_ValveTypeMixing

PSET_TYPEDRIVENOVERRIDE / IfcValve / MIXING

| A valve where typically the temperature of the outlet is determined by mixing hot and cold water inlet flows.
| 混合弁

buildingSMART Data Dictionary

PSD-XML

- MixerControl
  P_ENUMERATEDVALUE / IfcLabel / PEnum_MixingValveControl: MANUAL, PREDEFINED, THERMOSTATIC, OTHER, NOTKNOWN, UNSET

  | MixerControl: Defines the form of control of the mixing valve.
  | 混合制御: 混合弁の制御形式の定義

- OutletConnectionSize
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | OutletConnectionSize: The size of the pipework connection from the mixing valve.
  | 出力側接続口径: 混合弁の配管接続サイズ

Link to this page