#### 7.3.4.23 Pset_ValveTypeAirRelease

PSET_TYPEDRIVENOVERRIDE / IfcValve / AIRRELEASE

| Valve used to release air from a pipe or fitting. Note that an air release valve is constrained to have a single port pattern
| 弁タイプ空気抜き弁

buildingSMART Data Dictionary

PSD-XML

- IsAutomatic
  P_SINGLEVALUE / IfcBoolean

  | IsAutomatic: Indication of whether the valve is automatically operated (TRUE) or manually operated (FALSE).
  | 自動: 弁が自動(TRUE)で操作されるか手動(FALSE)で操作されるかの表示

Link to this page