#### 7.3.4.10 Pset_FlowMeterTypeEnergyMeter

PSET_TYPEDRIVENOVERRIDE / IfcFlowMeter / ENERGYMETER

| Device that measures, indicates and sometimes records, the energy usage in a system.

buildingSMART Data Dictionary

PSD-XML

- NominalCurrent
  P_SINGLEVALUE / IfcElectricCurrentMeasure

  | NominalCurrent: The nominal current that is designed to be measured.

- MaximumCurrent
  P_SINGLEVALUE / IfcElectricCurrentMeasure

  | MaximumCurrent: The maximum allowed current that a device is certified to handle.

- MultipleTarriff
  P_SINGLEVALUE / IfcBoolean

  | MultipleTarriff: Indicates whether meter has built-in support for multiple tarriffs (variable energy cost rates).

Link to this page