#### 6.4.4.2 Pset_SystemFurnitureElementTypePanel

PSET_TYPEDRIVENOVERRIDE / IfcSystemFurnitureElement / PANEL

| A set of specific properties for vertical panels that assembly workstations.. HISTORY: First issued in IFC Release R1.5. Renamed from Pset_Panel

buildingSMART Data Dictionary

PSD-XML

- HasOpening
  P_SINGLEVALUE / IfcBoolean

  | HasOpening: indicates whether the panel has an opening (= TRUE) or not (= FALSE).

- FurniturePanelType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_FurniturePanelType: ACOUSTICAL, GLAZED, HORZ_SEG, MONOLITHIC, OPEN, ENDS, DOOR, SCREEN, OTHER, NOTKNOWN, UNSET

  | FurniturePanelType: Available panel types from which that required may be selected.

- NominalThickness
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | NominalThickness: The nominal thickness of the panel.

Link to this page