#### 7.1.4.14 Pset_ControllerTypeProgrammable

PSET_TYPEDRIVENOVERRIDE / IfcController / PROGRAMMABLE

| Properties for Discrete Digital Control (DDC) or programmable logic controllers. HISTORY: Added in IFC4.

buildingSMART Data Dictionary

PSD-XML

- ControlType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_ControllerTypeProgrammable: PRIMARY, SECONDARY, OTHER, NOTKNOWN, UNSET

  | ControlType: The type of discrete digital controller: PRIMARY: Controller has built-in communication interface for PC connection, may manage secondary controllers. SECONDARY: Controller communicates with primary controller and its own managed devices.

- FirmwareVersion
  P_SINGLEVALUE / IfcLabel

  | FirmwareVersion: Indicates version of device firmware according to device manufacturer.
  | 펌웨어 버전: 컨트롤러 펌웨어 버전

- SoftwareVersion
  P_SINGLEVALUE / IfcLabel

  | SoftwareVersion: Indicates version of application software according to systems integrator.
  | 소프트웨어 버전: 컨트롤러 소프트웨어 버전

- Application
  P_ENUMERATEDVALUE / IfcLabel / PEnum_ControllerApplication: ModemController, TelephoneDirectory, FanCoilUnitController, RoofTopUnitController, UnitVentilatorController, SpaceConfortController, VAV, PumpController, BoilerController, DischargeAirController, OccupancyController, ConstantLightController, SceneController, PartitionWallController, RealTimeKeeper, RealTimeBasedScheduler, LightingPanelController, SunblindController, OTHER, NOTKNOWN, UNSET

  | Application: Indicates application of controller.

Link to this page