#### 7.1.4.32 Pset_SensorTypeLightSensor

PSET_TYPEDRIVENOVERRIDE / IfcSensor / LIGHTSENSOR

| A device that senses or detects light. HISTORY: LightSensorSensorSetPoint changed to SetPointIlluminance. Range, accuracy and time constant deleted.
| 光を感知または検出するデバイス。

buildingSMART Data Dictionary

PSD-XML

- SetPointIlluminance
  P_BOUNDEDVALUE / IfcIlluminanceMeasure

  | SetPointIlluminance: The illuminance value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.
  | 照度設定値: 感知される照度。 セットポイント値を置くために、IfcPropertyBoundedValue.SetPointValueを使用する。
  | 조도 설정: 감지하는 조도. 세트 포인트 값을 넣으려면, IfcPropertyBoundedValue.SetPointValue를 사용하십시오.

Link to this page